{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":11,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM40M2V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","","","30","34"]
["","","Apsilde","Sevišķi lēns","m³/min.","","","32","34"]
["Skaņas jaudas līmenis","Apsilde","","","dBA","","62","","","62"]
["","Dzesēšana","","","dBA","","60","","","60"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","cfm","","","1059","1200"]
["","","Apsilde","Sevišķi lēns","cfm","","","1130","1200"]
["Izmēri","Ierīce","","Augstums","mm","550","550","550","550","550","550"]
["","","","Platums","mm","765","765","765","765","765","765"]
["","","","Dziļums","mm","285","285","285","285","285","285"]
["Svars","Ierīce","","","kg","36","36","36","41","41","41"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","500","500","760","890","500","500"]
["","","Apsilde","Sevišķi lēns","apgr./min.","320","320","820","890","500","500"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","46.0","-10","-10","46.0"]
["","","","Maks.","°CDB","","-10","46","46","-10"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","-15","-15","-15","-15.0"]
["","","","Maks.","° CWB","","18.0","18","18","18.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","46","46","","","48","48"]
["","","","Nom.","dBA","","","48","46"]
["","Apsilde","","Augsta","dBA","48","48","","","50","50"]
["","","","Nom.","dBA","","","50","48"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Daudzums","","","kg","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Daudzums","","","tCO2Eq","0.59","0.6","0.6","0.8","0.78","0.78"]
["","GWP","","","","675.0","675","675","675","675","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20","20 (1)","20","20","20 (1)","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","002 (cauruļvadu garumam kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15.0","15","15","15","15","15.0"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5","7.5","7.5","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","30","30","30","30","30"]
["Standard Accessories","Installation manual","","","","1","1","Installation manual","1","1","1"]
["","Drain plug","","","","1","1","Drain plug","1","1","1"]
["","Screw bag","","","","1","1","Screw bag","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50","50","50"]
["","Spriegums","","","V","220-230-240","220-230-240","220-240","220-240","220-230-240","220-230-240"]
["Notes","","","","","(1) - Vienai telpai","","(1) - Satur fluorētas siltumnīcefekta gāzes","","","(1) - Vienai telpai"]
["","","","","","","(1) - Vienai telpai","","","(1) - Vienai telpai"]
["","","","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","","(4) - Satur fluorētas siltumnīcefekta gāzes","","","(4) - Satur fluorētas siltumnīcefekta gāzes"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Standard Accessories","Reducer assembly","","","","","","","1","1","1"]