{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-A8"]
[]
[]
[]
[]
["","","","","","2MXM50A2V1B8","2MXM68A2V1B8"]
["Izmēri","Ierīce","","Augstums","mm","552","734"]
["","","","Platums","mm","852","974"]
["","","","Dziļums","mm","350","408"]
["Svars","Ierīce","","","kg","41","60"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","50","50"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","48","48"]
["","Apsilde","","Nom.","dBA","50","48"]
["Aukstumaģents","Tips","","","","R-32","R-32"]
["","Daudzums","","","kg","1.15","2.00"]
["","Daudzums","","","tCO2Eq","0.78","1.35"]
["","GWP","","","","675","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20 (1)","25 (1)"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","002 (cauruļvadu garumam kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","50"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain cap","","","","","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Energoefektivitātes diapazons","","","","","A+++ ~ D","A+++ ~ D"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Notes","","","","","(1) - Vienai telpai","(1) - Vienai telpai"]
["","","","","","(2) - Izmantošanai apvienojumā ar CVXM-A, FVXM-A — maksimālais cauruļu sistēmas garums ir 30m.","(2) - Izmantošanai apvienojumā ar CVXM-A, FVXM-A — maksimālais cauruļu sistēmas garums ir 30m."]
["","","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","(5) - Satur fluorētas siltumnīcefekta gāzes","(5) - Satur fluorētas siltumnīcefekta gāzes"]