{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","30","","","34"]
["","","Apsilde","Sevišķi lēns","m³/min.","32","","","34"]
["","","","Sevišķi lēns","cfm","1059","","","1200"]
["","","Apsilde","Sevišķi lēns","cfm","1130","","","1200"]
["Izmēri","Ierīce","","Augstums","mm","550","550","550","550"]
["","","","Platums","mm","765","765","765","765"]
["","","","Dziļums","mm","285","285","285","285"]
["Svars","Ierīce","","","kg","36","36","36","41"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","760","500","500","890"]
["","","Apsilde","Sevišķi lēns","apgr./min.","820","320","320","890"]
["Compressor","Type","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10","-10 (2)","-10"]
["","","","Maks.","°CDB","46","46","46 (2)","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","46","46"]
["","","","Nom.","dBA","48","","","46"]
["","Apsilde","","Augsta","dBA","","48","48"]
["","","","Nom.","dBA","50","","","48"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32","R-32"]
["","Daudzums","","","kg","0.88","0.88","0.88","1.15"]
["","Daudzums","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20","20","20 (1)","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15.0","15.0","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","30","30","30"]
["Standard Accessories","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50"]
["","Spriegums","","","V","220-240","220-230-240","220-230-240","220-240"]
["Notes","","","","","","(1) - Vienai telpai"]
["","","","","","","","(1) - Vienai telpai"]
["","","","","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["Standard Accessories","Reducer assembly","","","","","","","1"]