{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M9"]
[]
[]
[]
[]
["","","","","","2MXM50M3V1B9","2MXM50M2V1B9"]
["Izmēri","Ierīce","","Augstums","mm","550","550"]
["","","","Platums","mm","765","765"]
["","","","Dziļums","mm","285","285"]
["Svars","Ierīce","","","kg","41","41"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","500","500"]
["","","Apsilde","Sevišķi lēns","apgr./min.","500","500"]
["Compressor","Type","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","48","48"]
["","Apsilde","","Augsta","dBA","50","50"]
["Aukstumaģents","Tips","","","","R-32","R-32"]
["","Daudzums","","","kg","1.15","1.15"]
["","Daudzums","","","tCO2Eq","0.78","0.8"]
["","GWP","","","","675","675.0"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15.0","15.0"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","30"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-230-240","220-230-240"]
["Notes","","","","","(1) - Vienai telpai","(1) - Katru D-AHU Professional var projektēt atbilstoši jūsu vajadzībām. Izvēlieties savu AHU vietnē tools.daikinapplied.eu"]