{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Izmēri","Ierīce","","Augstums","mm","550","550","734"]
["","","","Platums","mm","765","765","958"]
["","","","Dziļums","mm","285","285","340"]
["Svars","Ierīce","","","kg","36","41","60"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","500","500","420"]
["","","Apsilde","Sevišķi lēns","apgr./min.","320","500","420"]
["Kompresors","Type","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","46","48"]
["","","","Nom.","dBA","","","48"]
["","Apsilde","","Augsta","dBA","48","50"]
["","","","Nom.","dBA","","","48.0"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32"]
["","Daudzums","","","kg","0.88","1.15","2"]
["","Daudzums","","","tCO2Eq","0.60","0.78","1.35"]
["","GWP","","","","675","675","675.0"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20","20","25"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15.0","15.0","15.0"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","30","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-230-240","220-230-240","220-240"]
["Notes","","","","","(1) - Vienai telpai","(1) - Vienai telpai","(1) - Vienai telpai"]
["Standard Accessories","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]