{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXS-H"]
[]
[]
[]
[]
["","","","","","2MXS40H3V1B2","2MXS40H3V1B","2MXS40H2V1B","2MXS50H3V1B","2MXS50H3V1B2","2MXS50H2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","48","48","","50","50"]
["","Dzesēšana","","Nom.","dBA","47","47","","48","48"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1","","1","1"]
["","Skrūvju somiņa","","","","1","1","","1","1"]
["","Izplūdes aizbāznis","","","","1","1","","1","1"]
["Aukstumaģents","Charge","","","TCO2Eq","2.5","2.5","","3.3","3.3"]
["","GWP","","","","2,087.5","2,087.5","","2,087.5","2,087.5"]
["","Charge","","","kg","1.20","1.20","","1.60","1.60"]
["","Tips","","","","R-410A","R-410A","","R-410A","R-410A"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5","","7.5","7.5"]
["","","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15","","15","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","30","30","","30","30"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","765","765","","765","765"]
["","","","Dziļums","mm","285","285","","285","285"]
["","","","Augstums","mm","550","550","","550","550"]
["Svars","Ierīce","","","kg","38","38","","42","42"]
["Power supply","Fāze","","","","1~","1~","","1~","1~"]
["","Frekvence","","","Hz","50","50","","50","50"]
["","Spriegums","","","V","220-240","220-240","","220-240","220-240"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Satur fluorētas siltumnīcefekta gāzes","","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["Izmēri","Ierīce","","Augstums","mm","","","550","","","550"]
["","","","Platums","mm","","","765","","","765"]
["","","","Dziļums","mm","","","285","","","285"]
["Svars","Ierīce","","","kg","","","38","","","42"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","","10","","","10"]
["","","","Maks.","°CDB","","","46","","","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","","-15","","","-15"]
["","","","Maks.","° CWB","","","15.5","","","15.5"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","","47","","","48"]
["","Apsilde","","Nom.","dBA","","","48","","","50"]
["Aukstumaģents","Tips","","","","","","R-410A","","","R-410A"]
["","Daudzums","","","kg","","","1.20","","","1.60"]
["","Daudzums","","","tCO2Eq","","","2.5","","","3.3"]
["","GWP","","","","","","2087.5","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","","20","","","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","","","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)","","","0,02 (cauruļvadu garumam, kas pārsniedz 20 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","","15","","","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","","","7.5","","","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","","","30","","","30"]
["Standard Accessories","Installation manual","","","","","","1","","","1"]
["","Drain plug","","","","","","1","","","1"]
["","Screw bag","","","","","","1","","","1"]
["Barošanas avots","Fāze","","","","","","1~","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","50","","","50"]
["","Spriegums","","","V","","","220-240","","","220-240"]
["Standard Accessories","Pārejas montāža","","","","","","","1","1"]
["","Reducer assembly","","","","","","","","","1"]