{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","47"]
["","Dzesēšana","","Nom.","dBA","46"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Skrūvju somiņa","","","","1"]
["","Izplūdes aizbāznis","","","","1"]
["","Izplūdes vāks (1)","","","","6"]
["","Izplūdes vāks (2)","","","","3"]
["","Noņemama F-gas uzlīme","","","","1"]
["","Papildu dzesētāja uzlīme","","","","1"]
["Aukstumaģents","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Daudzums","","","kg","1.8"]
["","Tips","","","","R-32"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","420"]
["","","Apsilde","Sevišķi lēns","apgr./min.","420"]
["Piping connections","Līmeņa atšķirība","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5"]
["","","Iekštelpu ierīce – āra ierīce","Maks.","m","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","50"]
["Kompresors","Type","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","868"]
["","","","Dziļums","mm","320"]
["","","","Augstums","mm","734"]
["Svars","Ierīce","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["","","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","","24"]
["","","Apsilde","Sevišķi lēns","m³/min.","","24"]
["","","","Sevišķi lēns","cfm","","847"]
["","","Apsilde","Sevišķi lēns","cfm","","847"]
["Izmēri","Ierīce","","Augstums","mm","","734"]
["","","","Platums","mm","","868"]
["","","","Dziļums","mm","","320"]
["Svars","Ierīce","","","kg","","57"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","","420"]
["","","Apsilde","Sevišķi lēns","apgr./min.","","420"]
["Kompresors","Type","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","-10"]
["","","","Maks.","°CDB","","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","-15"]
["","","","Maks.","° CWB","","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","46"]
["","Apsilde","","Nom.","dBA","","47"]
["Aukstumaģents","Tips","","","","","R-32"]
["","Daudzums","","","kg","","1.80"]
["","Daudzums","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","25"]
["","Papildu dzesētāja uzlāde","","","kg/m","","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","","50"]
["Standard Accessories","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Barošanas avots","Fāze","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]