{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":8,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-M"]
[]
[]
[]
[]
["","","","","","3MXM40M2V1B","3MXM52M2V1B","3MXM68M2V1B"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","24","24","24.1"]
["","","Apsilde","Sevišķi lēns","m³/min.","24","24","24.1"]
["","","","Sevišķi lēns","cfm","847","847","851"]
["","","Apsilde","Sevišķi lēns","cfm","847","847","851"]
["Izmēri","Ierīce","","Augstums","mm","734","734","734"]
["","","","Platums","mm","868","868","868"]
["","","","Dziļums","mm","320","320","320"]
["Svars","Ierīce","","","kg","57","57","62"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","420","420"]
["","","Apsilde","Sevišķi lēns","apgr./min.","420","420"]
["Kompresors","Type","","","","Hermētiski noblīvēts šūpojošais kompresors","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","46","46","48"]
["","Apsilde","","Nom.","dBA","47","47","48"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32"]
["","Daudzums","","","kg","1.80","1.80","2.0"]
["","Daudzums","","","tCO2Eq","1.2","1.2","1.4"]
["","GWP","","","","675","675","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","25","25","25"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","50","50"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Standard Accessories","Drain cap","","","","","","9"]
["","Reducer assembly","","","","","","1"]