{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-K"]
[]
[]
[]
[]
["","","","","","3MXS40K3V1B","3MXS40K3V1B2","3MXS40K2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","47","47"]
["","Dzesēšana","","Nom.","dBA","46","46"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1"]
["","Izplūdes aizbāznis","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Uzlāde","","","kg","2.0","2.0"]
["","Type","","","","R-410A","R-410A"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5"]
["","","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","50","50"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","936","936"]
["","","","Depth","mm","300","300"]
["","","","Augstums","mm","735","735"]
["Svars","Ierīce","","","kg","49","49"]
["Power supply","Fāze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","230","230"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["Izmēri","Ierīce","","Augstums","mm","","","735"]
["","","","Platums","mm","","","936"]
["","","","Dziļums","mm","","","300"]
["Svars","Ierīce","","","kg","","","49"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Apsilde","Apkārtējā vide","Min.","°CWB","","","-15"]
["","","","Maks.","°CWB","","","15.5"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","","46"]
["","Apsilde","","Nom.","dBA","","","47"]
["Aukstumaģents","Tips","","","","","","R-410A"]
["","Daudzums","","","kg","","","2.0"]
["","Daudzums","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","","50"]
["","Papildu dzesētāja uzlāde","","","kg/m","","","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","","","7.5"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["Barošanas avots","Fāze","","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","50"]
["","Spriegums","","","V","","","230"]