{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":8,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXS-E"]
[]
[]
[]
[]
["","","","","","4MXS80E3V3B2","4MXS80E3V3B","4MXS80E7V3B"]
["Izmēri","Ierīce","","Augstums","mm","770","770"]
["","","","Platums","mm","900","900"]
["","","","Dziļums","mm","320","320"]
["Svars","Ierīce","","","kg","72","72"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15","-15"]
["","","","Maks.","° CWB","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","48","48"]
["","Apsilde","","Nom.","dBA","49","49"]
["Aukstumaģents","Tips","","","","R-410A","R-410A"]
["","Uzlāde","","","kg","2.99","2.99"]
["","GWP","","","","2,087.5","2,087.5"]
["Cauruļu savienojumi","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","7.5","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","70","70"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1"]
["","Izplūdes aizbāznis","","","","1","1"]
["","Pārejas montāža","","","","1","1"]
["Power supply","Fāze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","230","230"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5 m","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5 m","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5 m"]
["","","","","","(3) - Satur fluorētas siltumnīcefekta gāzes","(3) - Satur fluorētas siltumnīcefekta gāzes"]
["Izmēri","Ierīce","","Augstums","mm","","","770"]
["","","","Platums","mm","","","900"]
["","","","Dziļums","mm","","","320"]
["Svars","Ierīce","","","kg","","","72"]
["Kompresors","Veids","","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","","","-10"]
["","","","Maks.","°CDB","","","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","","","-15"]
["","","","Maks.","° CWB","","","15.5"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","","48"]
["","Apsilde","","Nom.","dBA","","","49"]
["Aukstumaģents","Tips","","","","","","R-410A"]
["","Daudzums","","","kg","","","2.99"]
["","Daudzums","","","tCO2Eq","","","6.2"]
["","GWP","","","","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","","","25"]
["","Papildu dzesētāja uzlāde","","","kg/m","","","0,02 (cauruļvadu garumam, kas pārsniedz 30 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","","15"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","","","7.5"]
["","Kopējais cauruļvadu garums","Sistēma","Faktiskais","m","","","70"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["Barošanas avots","Fāze","","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","50"]
["","Spriegums","","","V","","","230"]