{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","Uzstādīšanas rokasgrāmata"]
["","Lietošanas rokasgrāmata","","","","Lietošanas rokasgrāmata"]
["","Skrūve + paplāksne","","","","Skrūve + paplāksne"]
["","Bezvadu tālvadības pults","","","","Bezvadu tālvadības pults"]
["","Vāka slēdzējmehānisma režģis","","","","Vāka slēdzējmehānisma režģis"]
["","Baterija","","","","Baterija"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52"]
["","Gāze","","OD","mm","15.88"]
["","Aizplūde","","","","19.05"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.128"]
["","Apsilde","","Nom.","kW","0.128"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","64"]
["","Apsilde","","","dBA","64"]
["Izmēri","Ierīce","","Platums","mm","600"]
["","","","Dziļums","mm","1,007"]
["","","","Augstums","mm","285"]
["Korpuss","Materiāls","","","","Galvanizēts tērauds"]
["Svars","Ierīce","","","kg","35"]
["Ventilators","Ārējais statiskais spiediens","","Augsts","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Zems","Pa","64"]
["Power supply","Fāze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Nosaukums","","","","V1"]
["","Spriegums","","","V","220-240"]
["Strāvas ievade","Apsilde","","Nom.","kW","","0.109"]
["","Dzesēšana","","Nom.","kW","","0.109"]
["Ventilators","Ārējais statiskais spiediens","","Augsts","Pa","","70","150","150"]
["","","","Zems","Pa","","45","111","92"]
["Korpuss","Materiāls","","","","","Galvanizēts tērauds"]
["Izmēri","Ierīce","","Augstums","mm","","378","378","378"]
["","","","Platums","mm","","541","1300","1500"]
["","","","Dziļums","mm","","1045","541","541"]
["Svars","Ierīce","","","kg","","44","50","56"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","22.7","40.5","48.7"]
["","","","Nom.","m³/min.","","20.5","37","44"]
["","","","Zema","m³/min.","","18.3","34.8","37.9"]
["","","Apsilde","Augsta","m³/min.","","22.7","40.5","48.7"]
["","","","Nom.","m³/min.","","20.5","37.4","43.9"]
["","","","Zema","m³/min.","","18.3","34.8","37.9"]
["","Ārējais statiskais spiediens","","Nom.","Pa","","57","128","122"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","60","72","73"]
["","Apsilde","","","dBA","","60","72","73"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Zema","dBA","","36","50","50"]
["","Apsilde","","Augsta","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Zema","dBA","","36","50","50"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","9.52","9.52","9.52"]
["","Gāze","","OD","mm","","15.88","15.9","15.9"]
["","Aizplūde","","","","","19.05"]
["Standard Accessories","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Barošanas avots","Fāze","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","12.10","13.00"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","13.5","15.5"]
["Korpuss","Krāsa","","","","","","Cinkota tērauda plāksne / nekrāsota","Cinkota tērauda plāksne / nekrāsota"]
["Ventilators","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","","37","44"]
["","","Apsilde","Vidēja","m³/min.","","","37.4","43.9"]
["Skaņas spiediena līmenis","Dzesēšana","","Vidēja","dBA","","","52","53"]
["","Apsilde","","Vidēja","dBA","","","52","53"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","ARCWLA","ARCWLA"]