{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Klusa darbība","dBA","","36","","41"]
["","","","Zema","dBA","","38","","43"]
["","Dzesēšana","","Klusa darbība","dBA","","36","","41"]
["","","","Zema","dBA","","38","","43"]
["","","","Augsta","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","Uzstādīšanas rokasgrāmata","","Uzstādīšanas rokasgrāmata"]
["","Lietošanas rokasgrāmata","","","","","Lietošanas rokasgrāmata","","Lietošanas rokasgrāmata"]
["","Skrūves","","","","","Skrūves","","Skrūves"]
["","Paplāksne","","","","","Paplāksne","","Paplāksne"]
["","Bezvadu tālvadības pults","","","","","Bezvadu tālvadības pults","","Bezvadu tālvadības pults"]
["","Vāka slēdzējmehānisma režģis","","","","","Vāka slēdzējmehānisma režģis","","Vāka slēdzējmehānisma režģis"]
["","Baterija","","","","","Baterija","","Baterija"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Šķidrums","","OD","mm","","9.52","","9.52"]
["","Gāze","","OD","mm","","15.88","","15.88"]
["","Aizplūde","","","","","19.05","","19.05"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","","0.094","","0.137"]
["","Apsilde","","Nom.","kW","","0.094","","0.137"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","56","","60"]
["","Apsilde","","","dBA","","56","","60"]
["Izmēri","Ierīce","","Platums","mm","","820","","820"]
["","","","Dziļums","mm","","820","","820"]
["","","","Augstums","mm","","300","","300"]
["Korpuss","Materiāls","","","","","Galvanizēts tērauds","","Galvanizēts tērauds"]
["Svars","Ierīce","","","kg","","39","","39"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","","29.2","","34.0"]
["","","","Zema","m³/min.","","21.0","","26.3"]
["","","","Nom.","m³/min.","","24.4","","29.2"]
["","","Dzesēšana","Zema","m³/min.","","21.0","","26.3"]
["","","","Nom.","m³/min.","","24.4","","29.2"]
["","","","Augsta","m³/min.","","29.2","","34.0"]
["","","","Klusa darbība","m³/min.","","17.6","","22.1"]
["","","Dzesēšana","Klusa darbība","m³/min.","","17.6","","22.1"]
["Apdares panelis","Svars","","","kg","","4","","4"]
["","Izmēri","","Augstums","mm","","82","","82"]
["","","","Dziļums","mm","","990","","990"]
["","","","Platums","mm","","990","","990"]
["","Krāsa","","","","","Balts","","Balts"]
["Power supply","Fāze","","","","","1~","","1~"]
["","Nosaukums","","","","","V1","","V1"]
["","Frekvence","","","Hz","","50","","50"]
["","Spriegums","","","V","","220-240","","220-240"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Klusa darbība","m³/min.","15","","22.1"]
["Strāvas ievade","Apsilde","","Nom.","kW","0.067","","0.137"]
["","Dzesēšana","","Nom.","kW","0.067","","0.137"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Klusa darbība","m³/min.","15","","22.1"]
["Korpuss","Materiāls","","","","Galvanizēts tērauds","","Galvanizēts tērauds"]
["Izmēri","Ierīce","","Augstums","mm","265","","300"]
["","","","Platums","mm","820","","820"]
["","","","Dziļums","mm","820","","820"]
["Svars","Ierīce","","","kg","31","","39"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","24.4","","34"]
["","","","Nom.","m³/min.","20.5","","29.2"]
["","","","Zema","m³/min.","17.6","","26.3"]
["","","Apsilde","Augsta","m³/min.","24.4","","34"]
["","","","Nom.","m³/min.","20.5","","29.2"]
["","","","Zema","m³/min.","17.6","","26.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","54","","60"]
["","Apsilde","","","dBA","54","","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Zema","dBA","35","","43"]
["","","","Klusa darbība","dBA","32","","41"]
["","Apsilde","","Augsta","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Zema","dBA","35","","43"]
["","","","Klusa darbība","dBA","32","","41"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","","9.52"]
["","Gāze","","OD","mm","15.88","","15.88"]
["","Aizplūde","","","","19.05","","19.05"]
["Apdares panelis","Izmēri","","Augstums","mm","82","","82"]
["","","","Platums","mm","990","","990"]
["","","","Dziļums","mm","990","","990"]
["","Svars","","","kg","4","","4"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARCWLA","","ARCWLA"]
["","Tālv. pults ar vadu","","","","ARCWB","","ARCWB"]
["Standard Accessories","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Barošanas avots","Fāze","","","","1~","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","","50"]
["","Spriegums","","","V","220-240","","220-240"]