{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":6,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A / AZQS-B(8)V1"]
[]
[]
[]
[]
["","","","","ADEA100A2VEB / AZQS100B8V1B","ADEA125A2VEB / AZQS125B8V1B"]
["Dzesēšanas jauda","Nom.","","kW","9.50","12.10"]
["Telpu dzesēšana","SEER","","","5.10","4.83"]
["","Gada enerģijas patēriņš","","kWh/a","652","1,504"]
["","Jauda","Pdesign","kW","9.50","12.10"]
["","Energoefektivitātes klase","","","A"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","7.60","7.93"]
["","SCOP/A","","","3.81","3.50"]
["","Energoefektivitātes klase","","","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,793","3,167"]
["Nominālā efektivitāte","EER","","","","2.27"]
["Apsildes jauda","Nom.","","kW","10.80","13.50"]
["Notes","","","","(1) - Darbības diapazonu skatiet atsevišķā attēlā","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","(3) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","(3) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","(4) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","(4) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m"]