{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":11,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEA-A"]
[]
[]
[]
[]
["","","","","","ADEA35A2VEB","ADEA50A2VEB","ADEA60A2VEB","ADEA71A2VEB","ADEA100A2VEB","ADEA125A2VEB"]
["Ventilators","Ārējais statiskais spiediens","","Augsts","Pa","150","150","150","150","150","150"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","","","","14.00"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","","","","13.50"]
["Korpuss","Krāsa","","","","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)"]
["","Materiāls","","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["Izmēri","Ierīce","","Augstums","mm","245","245","245","245","245","245"]
["","","","Platums","mm","700","700","1000","1000","1400","1400"]
["","","","Dziļums","mm","800","800","800","800","800","800"]
["Svars","Ierīce","","","kg","28","28","35","35","46","46"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","15","15","18","18","29","34"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","12.5","12.5","15","15","26","29"]
["","","","Zema","m³/min.","10.5","10.5","12.5","12.5","23","23.5"]
["","","Apsilde","Augsta","m³/min.","15","15","18","18","29","34"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","12.5","12.5","15","15","26","29"]
["","","Apsilde","Zema","m³/min.","10.5","10.5","12.5","12.5","23","23.5"]
["","Ārējais statiskais spiediens","","Nom.","Pa","30","30","30","30","40","50"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60","60","56","56","58","62"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","35","35","30","30","34","37"]
["","","","Vidēja","dBA","32","32","28","28","32","35"]
["","","","Zema","dBA","29","29","25","25","30","32"]
["","Apsilde","","Augsta","dBA","37","37","31","31","36","38"]
["","","","Vidēja","dBA","34","34","28","28","33","35"]
["","","","Zema","dBA","29","29","25","25","30","32"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gāze","","OD","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Aizplūde","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Novadīšanas augstums","mm","","","","625","625","625","625","625","625"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Tālv. pults ar vadu","","","","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8"]
["","Operation manual","","","","1","1","1","","1","1"]
["","Clamps","","","","4","4","4","","4","4"]
["","Drain hose","","","","1","1","1","","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1"]
["","Screws","","","","40","40","40","","40","40"]
["","Sealing pads","","","","5","5","5","","5","5"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50","50","50"]
["","Spriegums","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","","","","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, ko rada skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, ko rada skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, ko rada skaņas avots."]
["","","","","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","","","1"]
["","Kronšteina skavas paplāksne","","","","","","","8"]
["","Lietošanas rokasgrāmata","","","","","","","1"]
["","Skavas","","","","","","","4"]
["","Izplūdes šļūtene","","","","","","","1"]
["","Piederumu izolācija","","","","","","","2"]
["","Izplūdes šļūtenes metāla skava","","","","","","","1"]
["","Skrūves","","","","","","","40"]
["","Blīvējuma paliktņi","","","","","","","5"]