{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ADEQ-C"]
[]
[]
[]
[]
["","","","","ADEQ35C2VEB","ADEQ50C2VEB","ADEQ60C2VEB","ADEQ71C2VEB","ADEQ100C2VEB","ADEQ125C2VEB"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","37","37","31","31","36","38"]
["","","Nom.","dBA","37","37","31","31","36","38"]
["","","Vidēja","dBA","34","34","28","28","33","35"]
["","","Zema","dBA","29","29","25","25","30","32"]
["","Dzesēšana","Vidēja","dBA","32","32","28","28","32","35"]
["","","Zema","dBA","29","29","25","25","30","32"]
["","","Augsta","dBA","35","35","30","30","34","37"]
["","","Nom.","dBA","35","35","30","30","34","37"]
["Standard Accessories","Lietošanas rokasgrāmata","","","1","1","1","1","1","1"]
["","Uzstādīšanas rokasgrāmata","","","1","1","1","1","1","1"]
["","Izplūdes šļūtene","","","1","1","1","1","1","1"]
["","Izplūdes šļūtenes metāla skava","","","1","1","1","1","1","1"]
["","Kronšteina skavas paplāksne","","","8","8","8","8","8","8"]
["","Skrūves","","","40","40","40","40","40","40"]
["","Piederumu izolācija","","","2","2","2","2","2","2"]
["","Blīvējuma paliktnis","","","5","5","5","5","5","5"]
["","Skavas","","","4","4","4","4","4","4"]
["Aukstumaģents","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5","2,087.5"]
["Dzesēšanas jauda","Kopējā jauda","Nom.","kW","","","","","","12.10"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52"]
["","Gāze","OD","mm","9.52","12.7","12.7","15.9","15.9","15.9"]
["","Izplūde","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Dzesēšana","","dBA","60","60","56","56","58","62"]
["Izmēri","Ierīce","Platums","mm","700","700","1,000","1,000","1,400","1,400"]
["","","Dziļums","mm","800","800","800","800","800","800"]
["","","Augstums","mm","245","245","245","245","245","245"]
["Korpuss","Materiāls","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["","Krāsa","","","Nekrāsots","Nekrāsots","Nekrāsots","Nekrāsots","Nekrāsots","Nekrāsots"]
["Svars","Ierīce","","kg","28.0","28.0","35.0","35","46","46"]
["Ventilators","Ārējais statiskais spiediens","Augsts","Pa","150","150","150","150","150","150"]
["","","Nom.","Pa","30","30","30","30","40","50"]
["Apsildes jauda","Kopējā jauda","Nom.","kW","","","","","","13.5"]
["Power supply","Fāze","","","1~","1~","1~","1~","1~","1~"]
["","Frekvence","","Hz","50","50","50","50","50","50"]
["","Spriegums","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots."]