{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":9,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AHQ-C"]
[]
[]
[]
[]
["","","","","","AHQ71CV1","AHQ100CV1","AHQ125CV1","AHQ140CV1"]
["Strāvas ievade","Apsilde","","Nom.","kW","0.106","0.149"]
["","Dzesēšana","","Nom.","kW","0.106","0.149"]
["Ventilators","Ārējais statiskais spiediens","","Augsts","Pa","0","0","0","0"]
["","","","Zems","Pa","0","0","0","0"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","12.10","13.00"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","13.5","15.5"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts","Balts"]
["","Materiāls","","","","Galvanizēts tērauds","Galvanizēts tērauds"]
["Izmēri","Ierīce","","Augstums","mm","260","260","260","285"]
["","","","Platums","mm","1320","1538","1790","1900"]
["","","","Dziļums","mm","634","634","634","680"]
["Svars","Ierīce","","","kg","38","45","65","70"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min.","21.3","27.8","31","39"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","","31","39"]
["","","","Zema","m³/min.","18.9","24.8","27.2","28.3"]
["","","Apsilde","Augsta","m³/min.","23.8","31.1","34.4","43.9"]
["","","","Nom.","m³/min.","21.3","27.8","30.6","39.1"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","","30.6","39.1"]
["","","Apsilde","Zema","m³/min.","18.9","24.8","27.2","28.3"]
["","Ārējais statiskais spiediens","","Nom.","Pa","0","0","0","0"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","59","64","65","71"]
["","Apsilde","","","dBA","62","64","65","71"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","49","52","52","56"]
["","","","Nom.","dBA","48","47"]
["","","","Vidēja","dBA","","","50","53"]
["","","","Zema","dBA","46","46","49","46"]
["","Apsilde","","Augsta","dBA","49","52","52","56"]
["","","","Vidēja","dBA","","","50","53"]
["","","","Nom.","dBA","48","47"]
["","","","Zema","dBA","46","46","49","46"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","9.52","9.52","9.52"]
["","Gāze","","OD","mm","15.88","15.88","15.9","15.9"]
["","Aizplūde","","","","19.05","19.05"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARCWLA","ARCWLA","ARCWLA","ARCWLA"]
["","Tālv. pults ar vadu","","","","ARCWB","ARCWB"]
["Standard Accessories","Installation manual","","","","Installation manual","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","Wireless remote control"]
["","Battery","","","","Battery","Battery"]
["","Noliešanas caurule","","","","Drain pipe","Drain pipe"]
["","Screw for wireless remote","","","","Screw for wireless remote","Screw for wireless remote"]
["","Ferrite Core","","","","Ferrite Core","Ferrite Core"]
["","Installation manual (Ferrite Core)","","","","Installation manual (Ferrite Core)","Installation manual (Ferrite Core)"]
["","Outdoor wiring diagram","","","","Outdoor wiring diagram","Outdoor wiring diagram"]
["","Operation manual","","","","Operation manual","Operation manual"]
["","Drain hose","","","","Drain hose","Drain hose"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]