{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M9"]
[]
[]
[]
[]
["","","","","","ARXM25M3V1B9","ARXM35M3V1B9","ARXM50M3V1B9"]
["Izmēri","Ierīce","","Augstums","mm","550","550","735"]
["","","","Platums","mm","765","765","825"]
["","","","Dziļums","mm","285","285","300"]
["Svars","Ierīce","","","kg","32","32","47"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","10","10","10"]
["","","","Maks.","° CWB","18","18","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","46","49","48"]
["","Apsilde","","Nom.","dBA","47","49","49"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32"]
["","Daudzums","","","kg","0.76","0.76","1.40"]
["","Daudzums","","","tCO2Eq","0.52","0.52","0.95"]
["","GWP","","","","675.0","675.0","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20.0","20.0","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","20.0","20.0","20"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240"]
["Notes","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Satur fluorētas siltumnīcefekta gāzes","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]