{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","","49.0"]
["","Dzesēšana","","Nom.","dBA","","49.0"]
["Standard Accessories","Izplūdes aizbāznis","","","","","1"]
["","Uzstādīšanas rokasgrāmata","","","","","1"]
["","Dzesētāja padeves marķējums","","","","","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","","1"]
["","Vispārēji drošības pasākumi","","","","","1"]
["Refrigerant","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Uzlāde","","","kg","","0.76"]
["","Tips","","","","","R-32"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Maks.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Cauruļvadu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","15"]
["","Papildu dzesētāja uzlāde","","","kg/m","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","","840"]
["","","","Dziļums","mm","","350"]
["","","","Augstums","mm","","552"]
["Svars","Ierīce","","","kg","","32"]
["Power supply","Fāze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]
["Notes","","","","","(1) - Iespējams tikai apvienojumā ar ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["","","","","","(2) - Iespējams tikai apvienojumā ar ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","","(4) - Iespējams tikai apvienojumā ar ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Iespējams tikai apvienojumā ar ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Izmēri","Ierīce","","Augstums","mm","552"]
["","","","Platums","mm","840"]
["","","","Dziļums","mm","350"]
["Svars","Ierīce","","","kg","32"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10"]
["","","","Maks.","°CDB","50 (4), 46 (5)"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","46.0"]
["","Apsilde","","Nom.","dBA","47.0"]
["Aukstumaģents","Daudzums","","","kg","0.76"]
["","Daudzums","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Strāvas padeve","Frekvence","","","Hz","50"]