{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":10,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)","ARXS60L2V1B (Archived)"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","","47","48"]
["","","","Nom.","dBA","","52","","","49"]
["","Dzesēšana","","Augsta","dBA","","","46","48"]
["","","","Nom.","dBA","","52","","","49"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","1","1","1","1"]
["","Izplūdes aizbāznis","","","","","1","1","1","1"]
["","Vairākvalodu fluorinēto siltumnīcu gāzu marķējumi","","","","","1","1","","1"]
["","Dzesētāja padeves marķējums","","","","","1","1","","1"]
["Aukstumaģents","Charge","","","TCO2Eq","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.70","1.0","1.2","1.50"]
["","Tips","","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","","","780","780"]
["","","Apsilde","Sevišķi lēns","apgr./min.","","","740","740"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Maks.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","10","10","-10"]
["","Apsilde","Apkārtējā vide","Maks.","° CWB","","18","18","18","18"]
["","","","Min.","° CWB","","-15","-15","-15","-15"]
["Cauruļu savienojumi","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","","20.0","15","15","20.0"]
["","Papildu dzesētāja uzlāde","","","kg/m","","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["Sound power level","Dzesēšana","","","dBA","","65","","","62"]
["","Apsilde","","","dBA","","65","","","62"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","","825","765","765","825"]
["","","","Dziļums","mm","","300","285","285","300"]
["","","","Augstums","mm","","735","550","550","735"]
["Svars","Ierīce","","","kg","","47","34","34","47"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Sevišķi lēns","cfm","","","904","904"]
["","","","Sevišķi lēns","m³/min.","","","25.6","25.6"]
["","","Dzesēšana","Sevišķi lēns","m³/min.","","","30.1","30.1"]
["","","","Sevišķi lēns","cfm","","","1,063","1,063"]
["Power supply","Fāze","","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","","50","50","50","50"]
["","Spriegums","","","V","","220-230-240","220-240","220-240","220-230-240"]
["Notes","","","","","","(1) - Satur fluorētas siltumnīcefekta gāzes","","","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","48.9"]
["","","Apsilde","Sevišķi lēns","m³/min.","43.1"]
["","","","Sevišķi lēns","cfm","1727"]
["","","Apsilde","Sevišķi lēns","cfm","1522"]
["Izmēri","Ierīce","","Augstums","mm","735"]
["","","","Platums","mm","825"]
["","","","Dziļums","mm","300"]
["Svars","Ierīce","","","kg","47"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","670"]
["","","Apsilde","Sevišķi lēns","apgr./min.","670"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","48"]
["","Apsilde","","Augsta","dBA","48"]
["Aukstumaģents","Tips","","","","R-410A"]
["","Daudzums","","","kg","1.7"]
["","Daudzums","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","20"]
["Standard Accessories","Installation manual","","","","1"]
["","Drain plug","","","","1"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - 220 V","","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus.","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus."]
["","","","","","(2) - 230 V","","(2) - 220 V","(2) - 220 V"]
["","","","","","(3) - 240 V","","(3) - 230 V","(3) - 230 V"]
["","","","","","","","(4) - 240 V","(4) - 240 V"]
["","","","","","","","(5) - Satur fluorētas siltumnīcefekta gāzes","(5) - Satur fluorētas siltumnīcefekta gāzes"]