{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","48"]
["","","","Zema","dBA","","45"]
["Standard Accessories","1","","","","","550"]
["Aukstumaģents","Charge","","","kg","","2.5"]
["","Tips","","","","","1.2"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","","30.1"]
["","","","Sevišķi lēns","cfm","","1,063"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","","740"]
["","","Apsilde","Sevišķi lēns","apgr./min.","","-15"]
["Darbības amplitūda","Apsilde","Apkārtējā vide","Min.","° CWB","","20"]
["","","","Maks.","° CWB","","10"]
["Skaņas spiediena līmenis","Dzesēšana","","Zema","dBA","","44"]
["","","","Augsta","dBA","","48"]
["Kompresors","Veids","","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Izmēri","Ierīce","","Platums","mm","","285"]
["","","","Dziļums","mm","","612"]
["","","","Augstums","mm","","765"]
["Svars","Ierīce","","","kg","","34"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Sevišķi lēns","cfm","","904"]
["","","","Sevišķi lēns","m³/min.","","25.6"]
["Power supply","Fāze","","","","","1~"]
["","Frekvence","","","Hz","","50"]
["","Spriegums","","","V","","220-240"]
["Notes","","","","","(1) - 220 V","(1) - Satur fluorētas siltumnīcefekta gāzes"]
["","","","","","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 230 V"]
["","","","","","","(4) - 240 V"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Sevišķi lēns","m³/min.","30.1"]
["","","Apsilde","Sevišķi lēns","m³/min.","25.6"]
["","","","Sevišķi lēns","cfm","1063"]
["","","Apsilde","Sevišķi lēns","cfm","904"]
["Izmēri","Ierīce","","Augstums","mm","550"]
["","","","Platums","mm","765"]
["","","","Dziļums","mm","285"]
["Svars","Ierīce","","","kg","34"]
["Ventilatora motors","Ātrums","Dzesēšana","Sevišķi lēns","apgr./min.","780"]
["","","Apsilde","Sevišķi lēns","apgr./min.","740"]
["Kompresors","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","10"]
["","","","Maks.","°CDB","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","46"]
["","Apsilde","","Augsta","dBA","47"]
["","","","Zema","dBA","44"]
["Aukstumaģents","Tips","","","","R-410A"]
["","Daudzums","","","kg","1.0"]
["","Daudzums","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","20"]
["","Papildu dzesētāja uzlāde","","","kg/m","0,02 (cauruļvadu garumam, kas pārsniedz 10 m)"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","15"]
["Standard Accessories","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]