{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","","","","","43"]
["","","","Vidēja","dBA","","","","","","35"]
["","","","Klusa darbība","dBA","","","","","","26"]
["","","","Zema","dBA","","","","","","29"]
["","Dzesēšana","","Vidēja","dBA","","","","","","34"]
["","","","Klusa darbība","dBA","","","","","","20"]
["","","","Zema","dBA","","","","","","27"]
["","","","Augsta","dBA","","","","","","43"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","","","","","1"]
["","Lietošanas rokasgrāmata","","","","","","","","","1"]
["","Infrasarkanā tālvadība","","","","","","","","","1"]
["","AA sausās baterijas","","","","","","","","","2"]
["","Tālvadības turētājs","","","","","","","","","1"]
["","Montāžas plāksne","","","","","","","","","1"]
["","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs","","","","","","","","","2"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","","","","","","2"]
["Vadības sistēmas","Wired remote control","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Cauruļvadu savienojumi","Šķidrums","","OD","mm","","","","","","6.35"]
["","Gāze","","OD","mm","","","","","","9.50"]
["","Izplūde","","","","","","","","","18"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","","","","","","0.024"]
["","Apsilde","","Nom.","kW","","","","","","0.029"]
["Sound power level","Dzesēšana","","","dBA","","","","","","58"]
["","Apsilde","","","dBA","","","","","","58"]
["Izmēri","Ierīce","","Platums","mm","","","","","","770"]
["","","","Dziļums","mm","","","","","","225"]
["","","","Augstums","mm","","","","","","286"]
["Korpuss","Krāsa","","","","","","","","","Balts"]
["Svars","Ierīce","","","kg","","","","","","9.0"]
["Power supply","Fāze","","","","","","","","","1~"]
["","Frekvence","","","Hz","","","","","","50"]
["","Nosaukums","","","","","","","","","V1"]
["","Spriegums","","","V","","","","","","220-240"]
["Notes","","","","","","","","","","(1) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Apsilde","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","286","286","286","286","286"]
["","","","Platums","mm","770","770","770","770","770"]
["","","","Dziļums","mm","225","225","225","225","225"]
["Svars","Ierīce","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9.9","9.9","10.4","10.4","11.8"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.8","7.8","8","8","8.2"]
["","","","Zema","m³/min.","5.8","5.8","6.1","6.1","6.3"]
["","","","Klusa darbība","m³/min.","4.8","4.8","4.8","4.8","4.9"]
["","","Apsilde","Augsta","m³/min.","10.9","10.9","11.1","11.1","12.8"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.5","8.5","8.5","8.5","8.5"]
["","","Apsilde","Zema","m³/min.","6.4","6.4","6.7","6.7","6.9"]
["","","","Klusa darbība","m³/min.","5.2","5.2","5.2","5.2","5.2"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","55","55","55","55","58"]
["","Apsilde","","","dBA","55","55","55","55","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","39","39","40","40","43"]
["","","","Vidēja","dBA","33","33","33","33","34"]
["","","","Zema","dBA","25","25","26","26","27"]
["","","","Klusa darbība","dBA","20","20","20","20","20"]
["","Apsilde","","Augsta","dBA","39","39","40","40","43"]
["","","","Vidēja","dBA","34","34","34","34","35"]
["","","","Zema","dBA","28","28","28","28","29"]
["","","","Klusa darbība","dBA","23","23","23","23","26"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Aizplūde","","","","18","18","18","18","18"]
["Vadības sistēmas","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Barošanas avots","Nosaukums","","","","V1","V1","V1","V1","V1"]
["","Fāze","","","","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","AAA dry-cell batteries","","","","","2","","2","2"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","ARC480A11","ARC480A11"]
["Standard Accessories","Titanium apatite photocatalytic air purification filter","","","","","","2"]