{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":87,"n_cols":11,"rows_kept":87,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-A"]
[]
[]
[]
[]
["","","","","","ATXF20A5V1B","ATXF50A2V1B","ATXF60A2V1B","ATXF71A2V1B","ATXF25A5V1B (Archived)","ATXF35A5V1B (Archived)"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","40","42","44","45"]
["","","","Vidēja","dBA","34","38","40","41"]
["","","","Klusa darbība","dBA","21","30","32","33"]
["","","","Zema","dBA","28","33","35","36"]
["","Dzesēšana","","Vidēja","dBA","33","39","41","42"]
["","","","Klusa darbība","dBA","20","31","33","34"]
["","","","Zema","dBA","26","34","36","37"]
["","","","Augsta","dBA","40","43","45","46"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1","1","1"]
["","Lietošanas rokasgrāmata","","","","1","1","1","1"]
["","Infrasarkanā tālvadība","","","","1","1","1","1"]
["","AAA sausās baterijas","","","","2","2","2","2"]
["","Tālvadības turētājs","","","","1","1","1","1"]
["","Montāžas plāksne","","","","1","1","1","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2","2","2","2"]
["Vadības sistēmas","Wired remote control","","","","BRC944B2, BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1"]
["Cauruļvadu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.50","12.7","12.7","12.7"]
["","Izplūde","","","","18","18","18","18"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.019","0.029","0.032","0.032"]
["","Apsilde","","Nom.","kW","0.020","0.032","0.035","0.035"]
["Sound power level","Dzesēšana","","","dBA","55","59","60","62"]
["","Apsilde","","","dBA","55","61","62","62"]
["Izmēri","Ierīce","","Platums","mm","770","990","990","990"]
["","","","Dziļums","mm","225","263","263","263"]
["","","","Augstums","mm","286","295","295","295"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts","Balts"]
["Svars","Ierīce","","","kg","8.50","13.5","13.5","13.5"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","10.3","17.3","17.9","17.9"]
["","","","Zema","m³/min.","6.7","12.2","12.8","12.8"]
["","","","Vidēja","m³/min.","8.6","14.8","15.8","15.8"]
["","","","Klusa darbība","m³/min.","5.3","10.7","11.3","11.3"]
["","","Dzesēšana","Zema","m³/min.","6.1","11.9","12.2","12.2"]
["","","","Vidēja","m³/min.","8.1","14.4","14.8","14.8"]
["","","","Augsta","m³/min.","10.1","16.8","17.3","17.3"]
["","","","Klusa darbība","m³/min.","4.4","10.5","10.7","10.7"]
["Power supply","Fāze","","","","1~","1~","1~","1~"]
["","Frekvence","","","Hz","50","50","50","50"]
["","Nosaukums","","","","","V1","V1","V1"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","","","","0.019","0.032"]
["","Apsilde","","Nom.","kW","","","","","0.02","0.032"]
["Korpuss","Krāsa","","","","","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","","","","286","286"]
["","","","Platums","mm","","","","","770","770"]
["","","","Dziļums","mm","","","","","225","225"]
["Svars","Ierīce","","","kg","","","","","8.5","9"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","","","","10.1","11.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","","","","8.1","8.3"]
["","","","Zema","m³/min.","","","","","6.1","6.3"]
["","","","Klusa darbība","m³/min.","","","","","4.4","4.5"]
["","","Apsilde","Augsta","m³/min.","","","","","10.3","11.5"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","","","","8.6","9"]
["","","Apsilde","Zema","m³/min.","","","","","6.7","7"]
["","","","Klusa darbība","m³/min.","","","","","5.3","5.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","","","","55","58"]
["","Apsilde","","","dBA","","","","","55","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","","","","40","43"]
["","","","Vidēja","dBA","","","","","33","34"]
["","","","Zema","dBA","","","","","26","27"]
["","","","Klusa darbība","dBA","","","","","20","20"]
["","Apsilde","","Augsta","dBA","","","","","40","40"]
["","","","Vidēja","dBA","","","","","34","35"]
["","","","Zema","dBA","","","","","28","29"]
["","","","Klusa darbība","dBA","","","","","21","21"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","","","","6.35","6.35"]
["","Gāze","","OD","mm","","","","","9.5","9.5"]
["","Aizplūde","","","","","","","","18","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","","","ARC470A1","ARC470A1"]
["","Tālv. pults ar vadu","","","","","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","","","","","1","1"]
["","AAA dry-cell batteries","","","","","","","","2","2"]
["","Operation manual","","","","","","","","1","1"]
["","Indoor unit fixing screws","","","","","","","","2","2"]
["","Infrared remote control","","","","","","","","1","1"]
["","Mounting plate","","","","","","","","1","1"]
["","Remote control holder","","","","","","","","1","1"]
["Barošanas avots","Fāze","","","","","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","","","50","50"]
["","Spriegums","","","V","","","","","220-240","220-240"]