{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-G"]
[]
[]
[]
[]
["","","","","","ATXF25G5V1B","ATXF35G5V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.023","0.029"]
["","Apsilde","","Nom.","kW","0.023","0.023"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","286","286"]
["","","","Platums","mm","770","770"]
["","","","Dziļums","mm","225","225"]
["Svars","Ierīce","","","kg","8.5","9"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9.8","10.9"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","8","7"]
["","","","Zema","m³/min.","6","5.7"]
["","","","Klusa darbība","m³/min.","4.3","4.6"]
["","","Apsilde","Augsta","m³/min.","10.4","9.3"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.4","7.5"]
["","","Apsilde","Zema","m³/min.","6.4","6"]
["","","","Klusa darbība","m³/min.","5.3","5.2"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","54","54"]
["","Apsilde","","","dBA","55","56"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","40","56"]
["","","","Vidēja","dBA","33"]
["","","","Zema","dBA","26"]
["","","","Klusa darbība","dBA","20"]
["","Apsilde","","Augsta","dBA","40","40"]
["","","","Vidēja","dBA","34","35"]
["","","","Zema","dBA","28","29"]
["","","","Klusa darbība","dBA","21","21"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6","6"]
["","Gāze","","OD","mm","9.5","9.5"]
["","Aizplūde","","","","18","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC480A93","ARC480A93"]
["","Tālv. pults ar vadu","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-440","220-440"]
["Notes","","","","","(1) - Dzesēšana: iekšējo temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 5m; līmeņa atšķirība: 0 m","(1) - Dzesēšana: iekšējo temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 5m; līmeņa atšķirība: 0 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m (horizontāli)","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m (horizontāli)"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]