{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":9,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-M"]
[]
[]
[]
[]
["","","","","","ATXM20M2V1B","ATXM25M2V1B","ATXM35M2V1B","ATXM50M2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.03","0.03","0.035","0.03"]
["","Apsilde","","Nom.","kW","0.025","0.025","0.025","0.032"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","294","294","294","300"]
["","","","Platums","mm","811","811","811","1040"]
["","","","Dziļums","mm","272","272","272","295"]
["Svars","Ierīce","","","kg","10","10","10","14.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","11.1","11.1","12.6","16.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.9","8.1","8.3","14.2"]
["","","","Zema","m³/min.","6","6.2","6.4","11.6"]
["","","","Klusa darbība","m³/min.","4.4","4.4","4.6","10.3"]
["","","Apsilde","Augsta","m³/min.","10.4","10.4","10.4","17.1"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.7","8.7","9","14.6"]
["","","Apsilde","Zema","m³/min.","6.5","6.8","7.1","12.2"]
["","","","Klusa darbība","m³/min.","5.3","5.3","5.3","10.7"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","58","58","60","59"]
["","Apsilde","","","dBA","55","55","55","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","41","41","45","44"]
["","","","Vidēja","dBA","33","33","33","40"]
["","","","Zema","dBA","25","25","29","36"]
["","","","Klusa darbība","dBA","19","19","19","32"]
["","Apsilde","","Augsta","dBA","39","39","39","43"]
["","","","Vidēja","dBA","34","34","35","39"]
["","","","Zema","dBA","26","27","28","34"]
["","","","Klusa darbība","dBA","20","20","20","31"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5","9.5","12.7"]
["","Aizplūde","","","","18","18","18","18"]
["Vadības sistēmas","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073"]
["Standard Accessories","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Barošanas avots","Nosaukums","","","","V1","V1","V1","V1"]
["","Fāze","","","","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240"]