{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R / ARXM-R9"]
[]
[]
[]
[]
["","","","","ATXM25R2V1B / ARXM25R5V1B9","ATXM25R5V1B / ARXM25R5V1B9","ATXM35R2V1B / ARXM35R5V1B9","ATXM35R5V1B / ARXM35R5V1B9"]
["Dzesēšanas jauda","Min.","","kW","","","1.40"]
["","Maks.","","kW","","","4.00"]
["","Nom.","","kW","","","3.40"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","","402"]
["","EER","","","","","4.23"]
["","COP","","","","","4.04"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","A"]
["","","Apsilde","","","","A"]
["Apsildes jauda","Nom.","","kW","","","4.00"]
["","Min.","","kW","","","1.40"]
["","Maks.","","kW","","","5.20"]
["Notes","","","","","","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Dzesēšanas jauda","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.50","2.50","","3.40"]
["","Maks.","","kW","3.20","3.20","","4.00"]
["Apsildes jauda","Min.","","kW","1.30","1.30","","1.40"]
["","Nom.","","kW","2.80","2.80","","4.00"]
["","Maks.","","kW","4.70","4.70","","5.20"]
["Nominālā efektivitāte","EER","","","4.50","4.50","","4.23"]
["","COP","","","5.00","5.00","","4.04"]
["","Gada enerģijas patēriņš","","kWh","278","278","","402"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","","A"]
["","","Apsilde","","A","A","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+++","A+++","","A+++"]
["","Jauda","Pdesign","kW","2.50","2.50","","3.40"]
["","SEER","","","8.55","8.55","","8.55"]
["","Gada enerģijas patēriņš","","kWh/a","102","102","","139"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A+++","A+++","","A+++"]
["","Jauda","Pdesign","kW","2.40","2.40","","2.50"]
["","SCOP/A","","","5.10","5.10","","5.10"]
["","Pdh Apsildes jauda pie -10°","","kW","2.30","2.30","","2.35"]
["","Gada enerģijas patēriņš","","kWh/a","659","659","","686"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]