{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":95,"n_cols":13,"rows_kept":95,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-R"]
[]
[]
[]
[]
["","","","","","ATXM20R2V1B §$ ATXM20R5V1B","ATXM20R2V1B","ATXM20R5V1B","ATXM25R2V1B","ATXM25R5V1B","ATXM35R2V1B","ATXM35R5V1B","ATXM50R2V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","39"]
["","","","Vidēja","dBA","34"]
["","","","Klusa darbība","dBA","20"]
["","","","Zema","dBA","26"]
["","Dzesēšana","","Vidēja","dBA","33"]
["","","","Klusa darbība","dBA","19"]
["","","","Zema","dBA","25"]
["","","","Augsta","dBA","41"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Bezvadu tālvadības pults","","","","1"]
["","AAA sausās baterijas","","","","2"]
["","Tālvadības turētājs","","","","1"]
["","Montāžas plāksne","","","","1"]
["","Titāna apatīta dezodorējošais filtrs","","","","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2"]
["","WLAN adaptera komplekts","","","","1"]
["Vadības sistēmas","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A67"]
["Cauruļvadu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.50"]
["","Izplūde","","","","18"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.029"]
["","Apsilde","","Nom.","kW","0.023"]
["Sound power level","Dzesēšana","","","dBA","58"]
["","Apsilde","","","dBA","55"]
["Izmēri","Ierīce","","Platums","mm","778"]
["","","","Dziļums","mm","272"]
["","","","Augstums","mm","295"]
["Korpuss","Krāsa","","","","Balts"]
["Svars","Ierīce","","","kg","10.0"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","9.3"]
["","","","Vidēja","m³/min.","8.2"]
["","","","Zema","m³/min.","6.2"]
["","","","Klusa darbība","m³/min.","5.1"]
["","","Dzesēšana","Zema","m³/min.","5.7"]
["","","","Vidēja","m³/min.","7.5"]
["","","","Augsta","m³/min.","10.5"]
["","","","Klusa darbība","m³/min.","4.3"]
["Power supply","Fāze","","","","1~"]
["","Nosaukums","","","","V1"]
["","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","0.029","0.029","0.029","0.029","0.03","0.03","0.03"]
["","Apsilde","","Nom.","kW","","0.023","0.023","0.022","0.022","0.027","0.027","0.032"]
["Korpuss","Krāsa","","","","","Balts","Balts","Balts","Balts","Balts","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","295","295","295","295","295","295","299"]
["","","","Platums","mm","","778","778","778","778","778","778","998"]
["","","","Dziļums","mm","","272","272","272","272","272","272","292"]
["Svars","Ierīce","","","kg","","10","10","10","10","10","10","14.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","10.5","10.5","10.5","10.5","11.3","11.3","15.8"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","7.5","7.5","7.6","7.6","7.8","7.8","14"]
["","","","Zema","m³/min.","","5.7","5.7","5.7","5.7","6","6","11.4"]
["","","","Klusa darbība","m³/min.","","4.3","4.3","4.1","4.1","4.2","4.2","8.3"]
["","","Apsilde","Augsta","m³/min.","","9.3","9.3","9.8","9.8","9.8","9.8","15.8"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","8.2","8.2","8","8","8.5","8.5","14.2"]
["","","Apsilde","Zema","m³/min.","","6.2","6.2","6.3","6.3","6.5","6.5","12"]
["","","","Klusa darbība","m³/min.","","5.1","5.1","4.9","4.9","4.9","4.9","10.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","58","58","58","58","58","58","58"]
["","Apsilde","","","dBA","","55","55","55","55","55","55","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","41","41","41","41","45","45","44"]
["","","","Vidēja","dBA","","33","33","33","33","33","33","40"]
["","","","Zema","dBA","","25","25","25","25","25","25","36"]
["","","","Klusa darbība","dBA","","19","19","19","19","19","19","27"]
["","Apsilde","","Augsta","dBA","","39","39","39","39","39","39","43"]
["","","","Vidēja","dBA","","34","34","34","34","35","35","39"]
["","","","Zema","dBA","","26","26","27","27","28","28","34"]
["","","","Klusa darbība","dBA","","20","20","20","20","20","20","31"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Gāze","","OD","mm","","9.5","9.5","9.5","9.5","9.5","9.5","12.7"]
["","Aizplūde","","","","","18","18","18","18","18","18","18"]
["Vadības sistēmas","Infrared remote control","","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","","1","1","1","1","1","1","1"]
["","Operation manual","","","","","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","1","1","1","1","1","1","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","1","1"]
["Barošanas avots","Nosaukums","","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Fāze","","","","","1~","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50","50","50","50","50","50","50"]
["","Spriegums","","","V","","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","Silver particle filter","","","","","","","","","","","1"]