{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-M"]
[]
[]
[]
[]
["","","","","","ATXP20M5V1B","ATXP25M5V1B","ATXP35M5V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.019","0.02","0.032"]
["","Apsilde","","Nom.","kW","0.023","0.023","0.032"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","286","286","286"]
["","","","Platums","mm","770","770","770"]
["","","","Dziļums","mm","225","225","225"]
["Svars","Ierīce","","","kg","8.5","8.5","9"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9.5","9.7","11.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.4","7.7","8.3"]
["","","","Zema","m³/min.","5.6","5.8","6.3"]
["","","","Klusa darbība","m³/min.","4.2","4.2","4.5"]
["","","Apsilde","Augsta","m³/min.","10.4","10.4","11.5"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.1","8.1","9"]
["","","Apsilde","Zema","m³/min.","6.2","6.4","7"]
["","","","Klusa darbība","m³/min.","5.2","5.2","5.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","55","55","58"]
["","Apsilde","","","dBA","55","55","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","39","40","43"]
["","","","Vidēja","dBA","33","33","34"]
["","","","Zema","dBA","25","26","27"]
["","","","Klusa darbība","dBA","19","19","20"]
["","Apsilde","","Augsta","dBA","39","40","40"]
["","","","Vidēja","dBA","34","34","35"]
["","","","Zema","dBA","28","28","29"]
["","","","Klusa darbība","dBA","21","21","21"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5","9.5"]
["","Aizplūde","","","","18","18","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC480A53","ARC480A53","ARC480A53"]
["","Tālv. pults ar vadu","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","2","2"]
["","Silver particle filter","","","","1"]
["","Indoor unit fixing screws","","","","2","2","2"]
["","Infrared remote control","","","","1","1","1"]
["","Mounting plate","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Barošanas avots","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240"]