{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":6,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","","AVA125AMVE"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","12.10"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","13.5"]
["Korpuss","Krāsa","","","","Dzidri balts"]
["Izmēri","Ierīce","","Augstums","mm","1850"]
["","","","Platums","mm","600"]
["","","","Dziļums","mm","350"]
["Svars","Ierīce","","","kg","50"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","28"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","26"]
["","","","Zema","m³/min.","24"]
["","","Apsilde","Augsta","m³/min.","28"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","26"]
["","","Apsilde","Zema","m³/min.","24"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","63"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","51"]
["","","","Vidēja","dBA","48"]
["","","","Zema","dBA","46"]
["","Apsilde","","Augsta","dBA","51"]
["","","","Vidēja","dBA","46"]
["","","","Nom.","dBA","48"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52"]
["","Gāze","","OD","mm","15.9"]
["","Aizplūde","","","","I.D. 20/O.D. 26"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Installation manual","","","","1"]
["","Hole protection rubber","","","","2"]
["","Cover","","","","1"]
["","Dew proof material","","","","1"]
["","Remote control wiring","","","","1"]
["","Bracket for installation","","","","1"]
["","Operation manual","","","","1"]
["","Bush","","","","1"]
["","Installation pattern","","","","1"]
["","Insulation for fitting for gas pipe","","","","1"]
["","Insulation for fitting for liquid pipe","","","","1"]
["","Screws","","","","5"]
["","Tie-wraps","","","","5"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50/60"]
["","Spriegums","","","V","220-240/220"]