{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AZAS-MV"]
[]
[]
[]
[]
["","","","","","AZAS100MUV","AZAS125MUV","AZAS140MUV"]
["Izmēri","Ierīce","","Augstums","mm","990","990","990"]
["","","","Platums","mm","940","940","940"]
["","","","Dziļums","mm","320","320","320"]
["Svars","Ierīce","","","kg","72","72","79"]
["Compressor","Veids","","","","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors","Hermētiski noblīvēts šūpojošais kompresors"]
["Darbības amplitūda","Dzesēšana","Apkārtējā vide","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46"]
["","Apsilde","Apkārtējā vide","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","15.5","15.5","15.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","70","71","73"]
["","Apsilde","","","dBA","","71 (1)","73 (1)"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","53","53","54"]
["","Apsilde","","Nom.","dBA","57","57","57"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32"]
["","Daudzums","","","kg","2.6","2.6","2.9"]
["","GWP","","","","675","675","675"]
["","Daudzums","","","tCO2Eq","1.76","1.76","1.96"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","9.52","9.52"]
["","Gāze","","OD","mm","15.9","15.9","15.9"]
["Cauruļvadu savienojumi","Cauruļvadu garums","Maks.","Ārējā ierīce — iekštelpu ierīce","m","30","30","30"]
["","","Sistēma","Ekvivalents","m","50","50","50"]
["","","","Neuzlādēts","m","30","30","30"]
["","Papildu dzesētāja uzlāde","","","kg/m","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu","Skatiet uzstādīšanas rokasgrāmatu"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","30","30","30"]
["","","Iekštelpu ierīce-iekštelpu ierīce","Maks.","m","0.5","0.5","0.5"]
["Standard Accessories","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Declaration of conformity","","","","2","2","2"]
["","Tie-wraps","","","","2","2","2"]
["Barošanas avots","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240"]
["Strāva — 50Hz","Maks. drošinātāja ampēri (MFA)","","","A","25","32","32"]
["Notes","","","","","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21","(1) - Saskaņā ar ENER Lot 21"]
["","","","","","(2) - Eiropas/starptautiskā tehniskā standarta limitu iestatījums saskaņotām strāvām, ko rada iekārta, kas savienota ar publiskās lietošanas zemsprieguma sistēmu ar ievades strāvu > 16 A un ≤ 75 A uz fāzi.","(2) - Eiropas/starptautiskā tehniskā standarta limitu iestatījums saskaņotām strāvām, ko rada iekārta, kas savienota ar publiskās lietošanas zemsprieguma sistēmu ar ievades strāvu > 16 A un ≤ 75 A uz fāzi.","(2) - Eiropas/starptautiskā tehniskā standarta limitu iestatījums saskaņotām strāvām, ko rada iekārta, kas savienota ar publiskās lietošanas zemsprieguma sistēmu ar ievades strāvu > 16 A un ≤ 75 A uz fāzi."]
["","","","","","(3) - Ssc: Īssavienojuma strāva","(3) - Ssc: Īssavienojuma strāva","(3) - Ssc: Īssavienojuma strāva"]
["","","","","","(4) - Eiropas/starptautiskā tehniskais standarts, kas nosaka ierobežojumus harmoniskām strāvām, ko rada iekārta, kas savienota ar koplietošanas zemsprieguma sistēmu ar ieejas strāvu > 16 A un <= 75 A uz fāzi.","(4) - Eiropas/starptautiskā tehniskais standarts, kas nosaka ierobežojumus harmoniskām strāvām, ko rada iekārta, kas savienota ar koplietošanas zemsprieguma sistēmu ar ieejas strāvu > 16 A un <= 75 A uz fāzi.","(4) - Eiropas/starptautiskā tehniskais standarts, kas nosaka ierobežojumus harmoniskām strāvām, ko rada iekārta, kas savienota ar koplietošanas zemsprieguma sistēmu ar ieejas strāvu > 16 A un <= 75 A uz fāzi."]