{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52W"]
[]
[]
[]
[]
["","","","","BRC1H52W."]
["Iepakojums","Materiāls","","","Pape"]
["","Svars","","kg","0.0850"]
["Vides temperatūra","Relatīvais mitrums <","","%","95"]
["","Krātuve","Min.","°C","-20"]
["","","Maks.","°C","70"]
["","Darbība","Min.","°C","-10"]
["","","Maks.","°C","50"]
["Izmēri","Ierīce iesaiņojumā","Platums","mm","217"]
["","","Augstums","mm","50"]
["","","Dziļums","mm","161"]
["","Ierīce","Platums","mm","85"]
["","","Dziļums","mm","25"]
["","","Augstums","mm","85"]
["Korpuss","Pogu pārsegs","","","Nē"]
["","Colour","","","Balts"]
["","Darbības LED","Krāsa","","Blue status indicator"]
["LCD","Veids","","","100 x 150 dots"]
["","Aizmugurgaismojums","Krāsa","","Balts"]
["","Izmēri","Platums","mm","28.0"]
["","","Augstums","mm","40.7"]
["Svars","Ierīce iesaiņojumā","","kg","0.317"]
["","Ierīce","","kg","0.110"]
["Vadu savienojumi","Vadojuma garums","Maks.","m","500"]