{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDS"]
[]
[]
[]
[]
["","","","","BRC1HHDAS (Archived)","BRC1HHDASA (Archived)"]
["Korpuss","Krāsa","","","Sudraba","Sudraba"]
["","Pogu pārsegs","","","Nē","Nē"]
["","Darbības LED","Krāsa","","Zils statusa indikators","Zils statusa indikators"]
["Izmēri","Ierīce","Augstums","mm","85","85"]
["","","Platums","mm","85","85"]
["","","Dziļums","mm","25","25"]
["","Ierīce iesaiņojumā","Augstums","mm","50","50"]
["","","Platums","mm","217","217"]
["","","Dziļums","mm","161","161"]
["Svars","Ierīce","","kg","0.110","0.110"]
["","Ierīce iesaiņojumā","","kg","0.317","0.317"]
["Iepakojums","Materiāls","","","Pape","Pape"]
["","Svars","","kg","0.0850","0.0850"]
["LCD","Veids","","","100 x 150 punkti","100 x 150 punkti"]
["","Izmēri","Augstums","mm","40.7","40.7"]
["","","Platums","mm","28.0","28.0"]
["","Aizmugurgaismojums","Krāsa","","Balts","Balts"]
["Vides temperatūra","Darbība","Min.","°C","-10","-10"]
["","","Maks.","°C","50","50"]
["","Krātuve","Min.","°C","-20","-20"]
["","","Maks.","°C","70","70"]
["","Vides temperatūra-=-Relatīvais mitrums <-=-%","","%","95","95"]
["Vadības sistēmas","Temperatūras regulēšanas klase","","","VI","VI"]
["","Ieguldījums telpu apsildes sezonas efektivitātē","","%","4.0","4.0"]
["Vadu savienojumi","Vadojuma garums","Maks.","m","500","500"]