{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH05AFV32","CHYHBH08AFV32"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts"]
["","Materiāls","","","","Pārklāts lokšņu metāls","Pārklāts lokšņu metāls","Pārklāts lokšņu metāls"]
["Izmēri","Ierīce","","Augstums","mm","902","902","902"]
["","","","Platums","mm","450","450","450"]
["","","","Dziļums","mm","164","164","164"]
["Svars","Ierīce","","","kg","30.0","30.0","30.0"]
["PED","Kategorija","","","","","Art3§3, Izslēgtas no PED darbības jomas saskaņā ar Direktīvas 97/23/EK 1. panta 3.6. punktu.","Art3§3, Izslēgtas no PED darbības jomas saskaņā ar Direktīvas 97/23/EK 1. panta 3.6. punktu."]
["Ūdens puses siltummainis","Ūdens plūsmas ātrums","Apsilde","Maks.","l/min.","23.0 (5)","23.0 (5)","23.0 (5)"]
["Skaņas jaudas līmenis","Nom.","","","dBA","42 (6)","42 (6)","42 (6)"]
["Darbības amplitūda","Apsilde","Ūdens puse","Min.","°C","25 (7)","25 (7)","25 (7)"]
["","","","Maks.","°C","50 (7)","50 (7)","50 (7)"]
["Barošanas avots","Nosaukums","","","","V3","V3","V3"]
["","Fāze","","","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50"]
["","Spriegums","","","V","230","230","230"]
["Vadu savienojumi","Savienojumam ar lietotāja saskarni","","Daudzums","","2","2","2"]
["","","","Piezīme","","no 0,75 mm² līdz 1,25 mm² (maks. garums 500 m)","no 0,75 mm² līdz 1,25 mm² (maks. garums 500 m)","no 0,75 mm² līdz 1,25 mm² (maks. garums 500 m)"]
["Notes","","","","","(1) - Tikai iekštelpu ierīcei","(1) - Tikai iekštelpu ierīcei","(1) - Tikai iekštelpu ierīcei"]
["","","","","","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boileris apiets","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boileris apiets","(2) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C), boileris apiets"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), boileris apiets","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), boileris apiets","(3) - DB/WB 7°C/6°C - LWC 45℃ (DT=5°C), boileris apiets"]
["","","","","","(4) - Min. required","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Boileris apiets","(5) - Boileris apiets","(5) - Boileris apiets"]
["","","","","","(6) - Saskaņās ar EN14825","(6) - Saskaņās ar EN14825","(6) - Saskaņās ar EN14825"]
["","","","","","(7) - *HYHB* un *HYKOMB33AA ekspluatācijas diapazonus skatiet ekspluatācijas diapazonu zīmējumā","(7) - *HYHB* un *HYKOMB33AA ekspluatācijas diapazonus skatiet ekspluatācijas diapazonu zīmējumā","(7) - *HYHB* un *HYKOMB33AA ekspluatācijas diapazonus skatiet ekspluatācijas diapazonu zīmējumā"]