{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","39"]
["","","Vidēja","dBA","32"]
["","","Klusa darbība","dBA","21"]
["","","Zema","dBA","25"]
["","Dzesēšana","Vidēja","dBA","32"]
["","","Klusa darbība","dBA","21"]
["","","Zema","dBA","25"]
["","","Augsta","dBA","39"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","1"]
["","Lietošanas rokasgrāmata","","","1"]
["","Gaisa filtrs","","","2"]
["","Infrasarkanā tālvadība","","","1"]
["","Attālā kontrollera montāžas plāksne","","","1"]
["","Skrūvju somiņa","","","1"]
["","Skrūvju pārsegs","","","1"]
["","AAA sausās baterijas","","","2"]
["","Vispārēji drošības pasākumi","","","1"]
["Aukstumaģents","GWP","","","675.0"]
["Vadības sistēmas","Tālv. pults ar vadu","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35"]
["","Gāze","OD","mm","9.50"]
["","Izplūde","","","18"]
["Power input","Dzesēšana","Nom.","kW","0.020"]
["","Apsilde","Nom.","kW","0.020"]
["Sound power level","Dzesēšana","","dBA","57"]
["Izmēri","Ierīce","Platums","mm","798"]
["","","Dziļums","mm","189"]
["","","Augstums","mm","295"]
["Korpuss","Krāsa","","","Melnais koks"]
["Svars","Ierīce","","kg","12"]
["Power supply","Fāze","","","1~"]
["","Frekvence","","Hz","50"]
["","Nosaukums","","","V1"]
["","Spriegums","","V","220-240"]