{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.02"]
["","Apsilde","","Nom.","kW","0.02"]
["Korpuss","Krāsa","","","","Sudraba"]
["Izmēri","Ierīce","","Augstums","mm","295"]
["","","","Platums","mm","798"]
["","","","Dziļums","mm","189"]
["Svars","Ierīce","","","kg","11.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","11"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","8.2"]
["","","","Zema","m³/min.","6.1"]
["","","","Klusa darbība","m³/min.","4.6"]
["","","Apsilde","Augsta","m³/min.","10.9"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.7"]
["","","Apsilde","Zema","m³/min.","6.4"]
["","","","Klusa darbība","m³/min.","4.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","57"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","21"]
["","Apsilde","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","21"]
["Aukstumaģents","GWP","","","","675"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.5"]
["","Aizplūde","","","","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC466A58"]
["","Tālv. pults ar vadu","","","","BRC073"]
["Standard Accessories","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Gaisa filtrs","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Barošanas avots","Nosaukums","","","","V1"]
["","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]