{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.020"]
["","Apsilde","","Nom.","kW","0.020"]
["Korpuss","Colour","","","","Melns"]
["Izmēri","Ierīce","","Augstums","mm","295"]
["","","","Platums","mm","798"]
["","","","Dziļums","mm","189"]
["Svars","Ierīce","","","kg","11.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","11.0"]
["","","","Vidēja","m³/min.","8.2"]
["","","","Zema","m³/min.","6.1"]
["","","","Klusa darbība","m³/min.","4.6"]
["","","Apsilde","Augsta","m³/min.","10.9"]
["","","","Vidēja","m³/min.","8.7"]
["","","","Zema","m³/min.","6.4"]
["","","","Klusa darbība","m³/min.","4.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","57"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","21"]
["","Apsilde","","Augsta","dBA","39"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","21"]
["Aukstumaģents","GWP","","","","675.0"]
["Piping connections","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.50"]
["","Aizplūde","","","","18"]
["Vadības sistēmas","Infrared remote control","","","","ARC466A85"]
["","Tālv. pults ar vadu","","","","BRC073A1"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Gaisa filtrs","","","","2"]
["","Infrasarkanā tālvadība","","","","1"]
["","Attālā kontrollera montāžas plāksne","","","","1"]
["","Skrūvju somiņa","","","","1"]
["","Skrūvju pārsegs","","","","2"]
["","AAA sausās baterijas","","","","2"]
["","Vispārēji drošības pasākumi","","","","1"]
["Power supply","Nosaukums","","","","V1"]
["","Fāze","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]