{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.029","0.029"]
["","Apsilde","","Nom.","kW","0.023","0.023"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","295","295"]
["","","","Platums","mm","778","778"]
["","","","Dziļums","mm","272","272"]
["Svars","Ierīce","","","kg","10","10"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","10.5","10.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.5","7.5"]
["","","","Zema","m³/min.","5.7","5.7"]
["","","","Klusa darbība","m³/min.","4.3","4.3"]
["","","Apsilde","Augsta","m³/min.","9.3","9.3"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.2","8.2"]
["","","Apsilde","Zema","m³/min.","6.2","6.2"]
["","","","Klusa darbība","m³/min.","5.1","5.1"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","57","57"]
["","Apsilde","","","dBA","54","54"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","41","41"]
["","","","Vidēja","dBA","33","33"]
["","","","Zema","dBA","25","25"]
["","","","Klusa darbība","dBA","19","19"]
["","Apsilde","","Augsta","dBA","39","39"]
["","","","Vidēja","dBA","34","34"]
["","","","Zema","dBA","26","26"]
["","","","Klusa darbība","dBA","20","20"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5"]
["","Aizplūde","","","","18","18"]
["Vadības sistēmas","Infrared remote control","","","","ARC466A67","ARC466A67"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC073A1","BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Barošanas avots","Nosaukums","","","","V1","V1"]
["","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]