{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","38","","41"]
["","","","Klusa darbība","dBA","21","","21"]
["","","","Zema","dBA","28","","30"]
["","Dzesēšana","","Klusa darbība","dBA","21","","21"]
["","","","Zema","dBA","25","","28"]
["","","","Augsta","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Dzesēšana","","Nom.","dBA","31","","35"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","","1"]
["","Lietošanas rokasgrāmata","","","","1","","1"]
["","Bezvadu tālvadības pults","","","","1","","1"]
["","Akumulatori","","","","2","","2"]
["","Tālvadības turētājs","","","","1","","1"]
["","Montāžas plāksne","","","","1","","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2","","2"]
["","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs","","","","2","","2"]
["Vadības sistēmas","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","","6.35"]
["","Gāze","","OD","mm","9.5","","9.5"]
["","Izplūde","","","","18","","18"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.040","","0.040"]
["","Apsilde","","Nom.","kW","0.040","","0.040"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","55","","59"]
["","Apsilde","","","dBA","56","","58"]
["Izmēri","Ierīce","","Platums","mm","780","","780"]
["","","","Dziļums","mm","215","","215"]
["","","","Augstums","mm","289","","289"]
["Korpuss","Krāsa","","","","Balts","","Balts"]
["Svars","Ierīce","","","kg","8","","8"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","","","10.1"]
["","","","Zema","m³/min.","","","6.3"]
["","","","Klusa darbība","m³/min.","","","4.3"]
["","","Dzesēšana","Zema","m³/min.","","","5.2"]
["","","","Augsta","m³/min.","","","9.2"]
["","","","Klusa darbība","m³/min.","","","3.9"]
["","","","Nom.","m³/min.","","","8.1"]
["","","Dzesēšana","Nom.","m³/min.","","","7.2"]
["Power supply","Fāze","","","","1~","","1~"]
["","Frekvence","","","Hz","50","","50"]
["","Nosaukums","","","","V1","","V1"]
["","Spriegums","","","V","220-240","","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","0.04","","0.040"]
["","Apsilde","","Nom.","kW","","0.04","","0.040"]
["Korpuss","Krāsa","","","","","Balts","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","289","","289"]
["","","","Platums","mm","","780","","780"]
["","","","Dziļums","mm","","215","","215"]
["Svars","Ierīce","","","kg","","8","","8.00"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","7.9","","9.2"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","6.3","","7.2"]
["","","","Zema","m³/min.","","4.7","","5.2"]
["","","","Klusa darbība","m³/min.","","3.9","","3.9"]
["","","Apsilde","Augsta","m³/min.","","9","","10.1"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","7.5","","8.1"]
["","","Apsilde","Zema","m³/min.","","6","","6.3"]
["","","","Klusa darbība","m³/min.","","4.3","","4.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","55","","59"]
["","Apsilde","","","dBA","","56","","58"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","37","","42"]
["","","","Vidēja","dBA","","31","","35"]
["","","","Zema","dBA","","25","","28"]
["","","","Klusa darbība","dBA","","21","","21"]
["","Apsilde","","Augsta","dBA","","38","","41"]
["","","","Vidēja","dBA","","33","","36"]
["","","","Zema","dBA","","28","","30"]
["","","","Klusa darbība","dBA","","21","","21"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35","","6.35"]
["","Gāze","","OD","mm","","9.5","","9.50"]
["","Aizplūde","","","","","18","","18"]
["Vadības sistēmas","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Standard Accessories","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Barošanas avots","Nosaukums","","","","","V1","","V1"]
["","Fāze","","","","","1~","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50","","50"]
["","Spriegums","","","V","","220-240","","220-240"]