{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Skaņas spiediena līmenis","Nom.","","","dBA","32.0 (6)"]
["Refrigerant","GWP","","","","2,090"]
["","Daudzums","","","kg","1.80"]
["","Tips","","","","R-410A"]
["Darbības amplitūda","Uzstādīšanas vieta","","Min.","°C","5.00"]
["","","","Maks.","°C","30.0"]
["","Apsilde","Ūdens puse","Maks.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Sāls šķīduma puse","","Min.","°C","-5.00"]
["","","","Maks.","°C","20.0"]
["","Sadzīves lietojuma karstais ūdens","Ūdens puse","Maks.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Strāvas ievade","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Sound power level","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Izmēri","Ierīce","","Platums","mm","600"]
["","","","Dziļums","mm","728"]
["","","","Augstums","mm","1,730"]
["Korpuss","Materiāls","","","","Pārklāts lokšņu metāls"]
["","Colour","","","","Balts"]
["Tvertne","Ūdens daudzums","","","l","180"]
["","Pretkorozijas aizsardzība","","","","Anods"]
["","Izolācija","","Siltuma zudumi","kWh/24 h","1.36 (4)"]
["Svars","Ierīce","","","kg","210"]
["Telpu apsilde","Mērena klimata ūdens izplūde 35°C","Vispārēji","ηs (telpu apsildes sezonas efektivitāte)","%","194"]
["","","","Telpu apsildes sezonas efekt. klase","","A+++"]
["","","","SCOP","","5.06"]
["","Mērena klimata ūdens izplūde 55°C","Vispārēji","Seasonal space heating eff. class","","A++"]
["","","","ηs (telpu apsildes sezonas efektivitāte)","%","139"]
["","","","SCOP","","3.68"]
["Apsildes jauda","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Maks.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Fāze","","","","3~"]
["","Nosaukums","","","","9W"]
["","Frekvence","","","Hz","50"]
["","Spriegums","","","V","400"]
["Strāva","Ieteicamie drošinātāji","","","A","25"]
["Notes","","","","","(1) - EWB/LWB 0°C/-3°C - LWC 35°C (DT=5°C)"]
["","","","","","(2) - EWB/LWB 0°C/-3°C - LWC 45℃ (DT=5°C)"]
["","","","","","(3) - ar 40% propilēnglikola"]
["","","","","","(4) - Siltuma zumdumi saskaņā ar EN12897"]
["","","","","","(5) - Iekļaujot cauruļvadu + PHE + dublēšanas sildītāju; izņemot paplašināšanas trauku"]
["","","","","","(6) - Skaņas spiediena līmenis tiek mērīts, izmantojot mikrofonu 1 m atstatumā no ierīces. Tā ir relatīva vērtība atbilstoši atstatumam un akustiskajai videi."]
["","","","","","(7) - Ar siltumsūkni"]
["","","","","","(8) - Ar siltumsūkni un palīgsildītāju"]
["","","","","","(9) - Ar palīgsildītāju"]