{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":10,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-D3 / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHSH04P30DA3 / ERGA04EAV3A","EHSH08P30DA3 / ERGA06EAV3A","EHSH08P50DA3 / ERGA06EAV3A","EHSH08P30DA3 / ERGA08EAV3A","EHSH08P50DA3 / ERGA08EAV3A"]
["Indoor unit","","","","","EHSH04P30DA3","EHSH08P30DA3","EHSH08P50DA3","EHSH08P30DA3","EHSH08P50DA3"]
["Apsildes jauda","Nom.","","","kW","4.30, 4.60","6.00, 5.90","6.00, 5.90","7.50, 7.80","7.50, 7.80"]
["Strāvas ievade","Apsilde","","Nom.","kW","0.840, 1.26","1.24, 1.69","1.24, 1.69","1.63, 2.23","1.63, 2.23"]
["COP","","","","","5.10, 3.65","4.85, 3.50","4.85, 3.50","4.60, 3.50","4.60, 3.50"]
["Mājsaimniecības karstā ūdens uzsildīšana","Vispārēji","","Deklarētais slodzes grafiks","","L","L","XL","L","XL"]
["","Mērens klimats","","Ūdens uzsildīšanas energoefektivitātes klase","","A+","A+","A","A+","A"]
["Telpu apsilde","Mērena klimata ūdens izplūde 55°C","Vispārēji","SCOP","","3.26","3.25","3.25","3.27","3.27"]
["","","","Telpu apsildes sezonas efekt. klase","","A++","A++","A++","A++","A++"]
["","Mērena klimata ūdens izplūde 35°C","Vispārēji","SCOP","","4.48","4.47","4.47","4.56","4.56"]
["","","","Telpu apsildes sezonas efekt. klase","","A+++","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - 1. nosacījums: dzesēšana Ta 35 °C - LWE 18 °C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. nosacījums: dzesēšana Ta 35 °C - LWE 18 °C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. nosacījums: dzesēšana Ta 35 °C - LWE 18 °C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. nosacījums: dzesēšana Ta 35 °C - LWE 18 °C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)","(1) - 1. nosacījums: dzesēšana Ta 35 °C - LWE 18 °C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 35 °C (DT = 5 °C)"]
["","","","","","(2) - 2. nosacījums: dzesēšana Ta 35 °C - LWE 7°C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 45°C (DT = 5 °C)","(2) - 2. nosacījums: dzesēšana Ta 35 °C - LWE 7°C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 45°C (DT = 5 °C)","(2) - 2. nosacījums: dzesēšana Ta 35 °C - LWE 7°C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 45°C (DT = 5 °C)","(2) - 2. nosacījums: dzesēšana Ta 35 °C - LWE 7°C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 45°C (DT = 5 °C)","(2) - 2. nosacījums: dzesēšana Ta 35 °C - LWE 7°C ( DT = 5 °C); Apsilde Ta DB/WB 7 °C/6 °C - LWC 45°C (DT = 5 °C)"]