{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E / ERGA-EVH7"]
[]
[]
[]
[]
["","","","","","EHSH08P30EF / ERGA08EAV3H7","EHSH08P50EF / ERGA08EAV3H7","EHSH08P50EG / ERGA08EAV3H7","EHSH08P30EG / ERGA08EAV3H7"]
["Iekštelpu ierīce","","","","","EHSH08P30EF","EHSH08P50EF","EHSH08P50EG","EHSH08P30EG"]
["Apsildes jauda","Nom.","","","kW","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Strāvas ievade","Apsilde","","Nom.","kW","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["COP","","","","","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)","4.60 (1), 3.50 (2)"]
["Mājsaimniecības karstā ūdens uzsildīšana","Vispārēji","","Deklarētais slodzes grafiks","","L","XL","XL","L"]
["","Mērens klimats","","Ūdens uzsildīšanas energoefektivitātes klase","","A+","A+","A+","A+"]
["Telpu apsilde","Mērena klimata ūdens izplūde 55°C","Vispārēji","SCOP","","3.32","3.32","3.32","3.32"]
["","","","Telpu apsildes sezonas efekt. klase","","A++","A++","A++","A++"]
["","Mērena klimata ūdens izplūde 35°C","Vispārēji","SCOP","","4.56","4.56","4.56","4.56"]
["","","","Telpu apsildes sezonas efekt. klase","","A+++","A+++","A+++","A+++"]
["Notes","","","","","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]
["Energoefektivitātes diapazons","","","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]