{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-E"]
[]
[]
[]
[]
["","","","","","EHSH04P30EG","EHSH08P30EG","EHSH08P50EG","EHSH04P30EF (Archived)","EHSH08P30EF (Archived)","EHSH08P50EF (Archived)"]
["Korpuss","Krāsa","","","","Balta (RAL9016) / melna (RAL9017)","Balta (RAL9016) / melna (RAL9017)","Balta (RAL9016) / melna (RAL9017)","Balta (RAL9016) / melna (RAL9017)","Balta (RAL9016) / melna (RAL9017)","Balta (RAL9016) / melna (RAL9017)"]
["","Materiāls","","","","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns"]
["Izmēri","Ierīce","","Augstums","mm","1891","1891","1910","1892","1892","1905"]
["","","","Platums","mm","594","594","792","594","594","792"]
["","","","Dziļums","mm","644","644","817","644","644","812"]
["Svars","Ierīce","","","kg","77.0","77.0","97.0","77","77","107"]
["PED","Kategorija","","","","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3","Art4.3"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675","675","675"]
["","Daudzums","","","kg","1.50","1.50","1.50","1.5","1.5","1.5"]
["Skaņas jaudas līmenis","Nom.","","","dBA","39","39","39","39","39","39"]
["Darbības amplitūda","Apsilde","Ūdens puse","Min.","°C","18","18","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65","65","65"]
["","Dzesēšana","Apkārtējā vide","Min.","°CDB","10","10","10","10","10","10"]
["","","Ūdens puse","Min.","°C","5","5","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22","22","22"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50","50","50"]
["","Spriegums","","","V","230","230","230","230","230","230"]
["Notes","","","","","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897"]