{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSX-D3"]
[]
[]
[]
[]
["","","","","","EHSX04P30DA3","EHSX04P50DA3","EHSX08P30DA3","EHSX08P50DA3"]
["Korpuss","Krāsa","","","","Balta (RAL9016) / tumši pelēka (RAL7011)","Balta (RAL9016) / tumši pelēka (RAL7011)","Balta (RAL9016) / tumši pelēka (RAL7011)","Balta (RAL9016) / tumši pelēka (RAL7011)"]
["","Materiāls","","","","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns","Triecienizturīgs polipropilēns"]
["Izmēri","Ierīce","","Augstums","mm","1891","1896","1891","1896"]
["","","","Platums","mm","595","790","595","790"]
["","","","Dziļums","mm","615","790","615","790"]
["Svars","Ierīce","","","kg","73.0","93.0","73.0","93.0"]
["PED","Kategorija","","","","pants 3.3","pants 3.3","pants 3.3","pants 3.3"]
["Aukstumaģents","Tips","","","","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0"]
["","Daudzums","","","kg","1.50","1.50","1.50","1.50"]
["Skaņas jaudas līmenis","Nom.","","","dBA","39","39","39","39"]
["Darbības amplitūda","Apsilde","Ūdens puse","Min.","°C","18","18","18","18"]
["","","","Maks.","°C","65","65","65","65"]
["","Dzesēšana","Apkārtējā vide","Min.","°CDB","10","10","10","10"]
["","","Ūdens puse","Min.","°C","5","5","5","5"]
["","","","Maks.","°C","22","22","22","22"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50"]
["","Spriegums","","","V","230","230","230","230"]
["Elektriskais sildītājs","Strāvas padeve","","Nosaukums","","3V / 9W","3V / 9W","3V / 9W","3V / 9W"]
["","","","Fāze","","1~ / 3~","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frekvence","Hz","50","50","50","50"]
["Notes","","","","","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897","(1) - Siltuma zumdumi saskaņā ar EN12897"]
["","","","","","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C","(2) - TKW = 10°C/TWW = 40°C/TSP = 50°C"]
["","","","","","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃","(3) - TKW = 10°C/TWW = 40°C/TSP = 60℃"]
["","","","","","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C","(4) - TKW = 10°C/TWW = 40°C/TSP = 65°C"]
["","","","","","","(5) - Tvertnes uzsildīšana tikai ar siltummaini, bez elektriskā sildītāja","","(5) - Tvertnes uzsildīšana tikai ar siltummaini, bez elektriskā sildītāja"]