{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVH-E6V / ERGA-EV"]
[]
[]
[]
[]
["","","","","","EHVH04S18EA6V / ERGA04EAV3","EHVH04S18EJ6V / ERGA04EAV3","EHVH04S23EA6V / ERGA04EAV3","EHVH04S23EJ6V / ERGA04EAV3"]
["Apsildes jauda","Nom.","","","kW","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)","4.30 (1), 4.60 (2)"]
["Strāvas ievade","Apsilde","","Nom.","kW","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)","0.850 (1), 1.26 (2)"]
["Jaudas izlietojums","Mājsaimniecības karstais ūdens no 10°C līdz 50°C","","Nom.","kWh","2.48","2.48","3.01","3.01"]
["Uzsildīšanas laiks no 10°C līdz 50°C","hr","","","","1 h 28 min.","1 h 28 min.","1 h 40 min.","1 h 40 min."]
["COP","","","","","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)","5.10 (1), 3.65 (2)"]
["Mājsaimniecības karstā ūdens uzsildīšana","Vispārēji","","Deklarētais slodzes grafiks","","L","L","XL","XL"]
["","Mērens klimats","","Ūdens uzsildīšanas energoefektivitātes klase","","A+","A+","A+","A+"]
["Telpu apsilde","Mērena klimata ūdens izplūde 55°C","Vispārēji","SCOP","","3.26","3.26","3.26","3.26"]
["","","","Telpu apsildes sezonas efekt. klase","","A++","A++","A++","A++"]
["","Mērena klimata ūdens izplūde 35°C","Vispārēji","SCOP","","4.48","4.48","4.48","4.48"]
["","","","Telpu apsildes sezonas efekt. klase","","A+++","A+++","A+++","A+++"]
["Energoefektivitātes diapazons","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notes","","","","","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - 1. nosacījums: dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - 2. nosacījums: dzesēšana Ta 35°C - LWE 7°C ( DT = 5°C); Apsilde Ta DB/WB 7°C/6°C - LWC 45°C (DT = 5°C)"]