{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERGA-EV"]
[]
[]
[]
[]
["","","","","","ERGA04EAV3"]
["Izmēri","Ierīce","","Augstums","mm","740"]
["","","","Platums","mm","884"]
["","","","Dziļums","mm","388"]
["Svars","Ierīce","","","kg","58.5"]
["Darbības diapazons","Dzesēšana","","Min.","°CDB","10"]
["","","","Maks.","°CDB","43"]
["Darbības amplitūda","Sadzīves lietojuma karstais ūdens","","Min.","°CDB","-25"]
["Darbības diapazons","Mājsaimniecības karstais ūdens","","Maks.","°CDB","35"]
["Skaņas jaudas līmenis","Apsilde","","Nom.","dBA","58 (1)"]
["","Dzesēšana","","Nom.","dBA","61 (1)"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","44 (1)"]
["","Dzesēšana","","Nom.","dBA","48 (1)"]
["Aukstumaģents","Tips","","","","R-32"]
["","GWP","","","","675.0"]
["","Daudzums","","","tCO2Eq","1.01"]
["","Daudzums","","","kg","1.50"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6"]
["","Gāze","","OD","mm","15.9"]
["Cauruļvadu savienojumi","Izplūde","","OD","mm","18"]
["","Līmeņa atšķirība","Iekštelpu ierīce – āra ierīce","Maks.","m","20.0"]
["Cauruļu savienojumi","Siltumizolācija","","","","Šķidruma un gāzes cauruļvadi"]
["Barošanas avots","Nosaukums","","","","V3"]
["","Fāze","","","","1N~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","230"]
["Strāva","Ieteicamie drošinātāji","","","A","20"]
["Notes","","","","","(1) - Dzesēšana Ta 35°C - LWE 18°C ( DT = 5°C) Apsilde Ta DB/WB 7°C/6°C - LWC 35°C (DT = 5°C)"]