{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B"]
["Dzesēšanas jauda","Nom.","","kW","","","","6.80","6.80"]
["Telpu dzesēšana","SEER","","","","","","6.43","6.43"]
["","Gada enerģijas patēriņš","","kWh/a","","","","371","371"]
["","Jauda","Pdesign","kW","","","","6.80","6.80"]
["","Energoefektivitātes klase","","","","","","A++","A++"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","","","","6.33","6.33"]
["","SCOP/A","","","","","","4.02","4.02"]
["","Energoefektivitātes klase","","","","","","A+","A+"]
["","Gada enerģijas patēriņš","","kWh/a","","","","2,205","2,205"]
["Nominālā efektivitāte","EER","","","","","","3.40","3.40"]
["","Gada enerģijas patēriņš","","kWh","","","","1,000"]
["","COP","","","","","","3.70"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","","A"]
["","","Apsilde","","","","","A"]
["Apsildes jauda","Nom.","","kW","","","","7.50"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]