{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAA71BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG71L8Y1B","FAA100BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG100L8Y1B","FAA71BUV1B / FAA71BUV1B / RZQG125L8Y1B"]
["Dzesēšanas jauda","Nom.","","kW","6.80","6.80","9.50","9.50","12.00"]
["Telpas dzesēšana","SEER","","","6.43","6.43","6.11","5.10","5.10"]
["","Gada enerģijas patēriņš","","kWh/a","371","371","545","652","824"]
["","Jauda","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Energoefektivitātes klase","","","A++","A++","A++","A","A"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.33","6.33","10.20","11.30","12.71"]
["","SCOP/A","","","4.02","4.02","4.01","3.80","3.80"]
["","Energoefektivitātes klase","","","A+","A+","A+","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,205","2,205","3,562","4,164","4,683"]
["Nominālā efektivitāte","EER","","","3.40","3.40","3.62","3.75","3.61"]
["","Gada enerģijas patēriņš","","kWh","1,000","","1,312"]
["","COP","","","3.70","","3.61"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","","A"]
["","","Apsilde","","A","","A"]
["Apsildes jauda","Nom.","","kW","7.50","","10.80"]
["Notes","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Darbības diapazonu skatiet atsevišķā attēlā","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Darbības diapazonu skatiet atsevišķā attēlā","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Elektrības datus skatiet atsevišķā zīmējumā","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]