{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["","Materiāls","","","","Mastika","Mastika"]
["Izmēri","Ierīce","","Augstums","mm","290","340"]
["","","","Platums","mm","1050","1200"]
["","","","Dziļums","mm","269","262"]
["Svars","Ierīce","","","kg","14","18"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","16.2","23"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","13.4","21.1"]
["","","","Zema","m³/min.","12.1","18.7"]
["","","Apsilde","Augsta","m³/min.","16.9","23"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","14.2","20.9"]
["","","Apsilde","Zema","m³/min.","12.7","18.7"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","61","65"]
["","Apsilde","","","dBA","61","65"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","45","49"]
["","","","Vidēja","dBA","42","45"]
["","","","Zema","dBA","40","41"]
["","Apsilde","","Augsta","dBA","45","49"]
["","","","Vidēja","dBA","42","45"]
["","","","Zema","dBA","40","41"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","9.52"]
["","Gāze","","OD","mm","15.9","15.9"]
["","Aizplūde","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Barošanas avots","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Standard Accessories","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Notes","","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Standard Accessories","Screw cover","","","","","3"]