{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9 / RZQG71L8Y1B","FAQ100CVEB9 / RZQG71L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG100L8Y1B","FAQ100CVEB9 / RZQG100L8Y1B","FAQ71CVEB9 / FAQ71CVEB9 / RZQG125L8Y1B"]
["Dzesēšanas jauda","Nom.","","kW","6.8","","","9.5"]
["Telpas dzesēšana","SEER","","","6.43","6.51","5.10","6.11","5.10"]
["","Gada enerģijas patēriņš","","kWh/a","371","366","652","545","824"]
["","Jauda","Pdesign","kW","6.80","6.80","9.50","9.50","12.00"]
["","Energoefektivitātes klase","","","A++","A++","B","A++","B"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.33","6.33","11.30","10.20","12.71"]
["","SCOP/A","","","4.02","4.02","3.80","4.01","3.80"]
["","Energoefektivitātes klase","","","A+","A+","A","A+","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,205","2,205","4,164","3,562","4,683"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","1,000","","","1,315"]
["","EER","","","3.40","","","3.62"]
["","COP","","","3.70","","","3.61"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","","","A"]
["","","Apsilde","","A","","","A"]
["Apsildes jauda","Nom.","","kW","7.5","","","10.8"]
["Notes","","","","(1) - Ikgadējais enerģijas patēriņš atbilst Energomarķējuma direktīvai 2002/31/EK","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - SEER un SCOP atbilst EN 14825","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["","","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]