{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["","","Vidēja","dBA","42","45"]
["","","Zema","dBA","40","41"]
["","Dzesēšana","Vidēja","dBA","42","45"]
["","","Zema","dBA","40","41"]
["","","Augsta","dBA","45","49"]
["","","Nom.","dBA","42","45"]
["Dzesēšanas jauda","Kopējā jauda","Nom.","kW","0.051","0.061"]
["Piping connections","Šķidrums","OD","mm","9.52","9.52"]
["","Gāze","OD","mm","15.9","15.9"]
["","Izplūde","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","61","65"]
["","Apsilde","","dBA","61","65"]
["Izmēri","Ierīce","Platums","mm","1,050","1,200"]
["","","Dziļums","mm","238","240"]
["","","Augstums","mm","290","340"]
["Korpuss","Materiāls","","","Mastika","Mastika"]
["","Colour","","","Dzidri balts","Dzidri balts"]
["Svars","Ierīce","","kg","13","17"]
["Apsildes jauda","Kopējā jauda","Nom.","kW","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Spriegums","","V","220-240","220-240"]