{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / RXS-L"]
[]
[]
[]
[]
["","","","","FBA50A2VEB9 / RXS50L2V1B","FBA60A2VEB9 / RXS60L2V1B"]
["Dzesēšanas jauda","Nom.","","kW","","5.70"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","826"]
["","EER","","","","3.45"]
["","COP","","","","37.10"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","A"]
["","","Apsilde","","","A"]
["Apsildes jauda","Nom.","","kW","","7.00"]
["Notes","","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Āra ierīce","","","","RXS50L2V1B"]
["Dzesēšanas jauda","Nom.","","kW","5.00"]
["Apsildes jauda","Nom.","","kW","5.50"]
["Nominālā efektivitāte","EER","","","3.52"]
["","COP","","","38.30"]
["","Gada enerģijas patēriņš","","kWh","710"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A++"]
["","Jauda","Pdesign","kW","5.00"]
["","SEER","","","6.21"]
["","Gada enerģijas patēriņš","","kWh/a","282"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A+"]
["","Jauda","Pdesign","kW","4.40"]
["","SCOP/A","","","4.06"]
["","Pdh Apsildes jauda pie -10°","","kW","3.73"]
["","Gada enerģijas patēriņš","","kWh/a","1517"]
["Energoefektivitātes diapazons","","","","A+++ ~ D"]